(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu16.04.1)

  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 323)
    (zones 0)
    (modules 29)
    (nets 62)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 1)
    (trace_clearance 0.3)
    (zone_clearance 1)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 GNDD)
  (net 2 +5V)
  (net 3 RESET)
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C5-Pad2)")
  (net 6 "Net-(C6-Pad2)")
  (net 7 VCC)
  (net 8 MOSI)
  (net 9 SCK)
  (net 10 SS)
  (net 11 MISO)
  (net 12 /3v3)
  (net 13 TX)
  (net 14 RX)
  (net 15 ENCODER_B)
  (net 16 ENCODER_A)
  (net 17 ENCODER_BUTTON)
  (net 18 "Net-(J5-Pad2)")
  (net 19 "Net-(J5-Pad1)")
  (net 20 +9V)
  (net 21 SERVO_SLIDER)
  (net 22 "Net-(J8-Pad1)")
  (net 23 "Net-(J8-Pad2)")
  (net 24 "Net-(J8-Pad3)")
  (net 25 "Net-(J8-Pad4)")
  (net 26 "Net-(J8-Pad5)")
  (net 27 "Net-(J8-Pad6)")
  (net 28 "Net-(J8-Pad7)")
  (net 29 "Net-(J8-Pad8)")
  (net 30 SRDATA)
  (net 31 SRCLOCK)
  (net 32 SRLATCH)
  (net 33 MOTOR_1)
  (net 34 MOTOR_2)
  (net 35 "Net-(U4-Pad1)")
  (net 36 "Net-(U4-Pad2)")
  (net 37 "Net-(U4-Pad3)")
  (net 38 "Net-(U4-Pad4)")
  (net 39 "Net-(U4-Pad5)")
  (net 40 "Net-(U4-Pad6)")
  (net 41 "Net-(U4-Pad7)")
  (net 42 "Net-(U4-Pad15)")
  (net 43 "Net-(U5-Pad15)")
  (net 44 "Net-(U5-Pad7)")
  (net 45 "Net-(U5-Pad6)")
  (net 46 "Net-(U5-Pad5)")
  (net 47 "Net-(U5-Pad4)")
  (net 48 "Net-(U5-Pad3)")
  (net 49 "Net-(U5-Pad2)")
  (net 50 "Net-(U5-Pad1)")
  (net 51 "Net-(J6-Pad8)")
  (net 52 "Net-(J6-Pad7)")
  (net 53 "Net-(J6-Pad6)")
  (net 54 "Net-(J6-Pad5)")
  (net 55 "Net-(J6-Pad4)")
  (net 56 "Net-(J6-Pad3)")
  (net 57 "Net-(J6-Pad2)")
  (net 58 "Net-(J6-Pad1)")
  (net 59 GNDPWR)
  (net 60 "Net-(U4-Pad14)")
  (net 61 "Net-(J9-Pad3)")

  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net +9V)
    (add_net /3v3)
    (add_net ENCODER_A)
    (add_net ENCODER_B)
    (add_net ENCODER_BUTTON)
    (add_net GNDD)
    (add_net GNDPWR)
    (add_net MISO)
    (add_net MOSI)
    (add_net MOTOR_1)
    (add_net MOTOR_2)
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(J6-Pad5)")
    (add_net "Net-(J6-Pad6)")
    (add_net "Net-(J6-Pad7)")
    (add_net "Net-(J6-Pad8)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(J8-Pad3)")
    (add_net "Net-(J8-Pad4)")
    (add_net "Net-(J8-Pad5)")
    (add_net "Net-(J8-Pad6)")
    (add_net "Net-(J8-Pad7)")
    (add_net "Net-(J8-Pad8)")
    (add_net "Net-(J9-Pad3)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad14)")
    (add_net "Net-(U4-Pad15)")
    (add_net "Net-(U4-Pad2)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U4-Pad7)")
    (add_net "Net-(U5-Pad1)")
    (add_net "Net-(U5-Pad15)")
    (add_net "Net-(U5-Pad2)")
    (add_net "Net-(U5-Pad3)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U5-Pad6)")
    (add_net "Net-(U5-Pad7)")
    (add_net RESET)
    (add_net RX)
    (add_net SCK)
    (add_net SERVO_SLIDER)
    (add_net SRCLOCK)
    (add_net SRDATA)
    (add_net SRLATCH)
    (add_net SS)
    (add_net TX)
    (add_net VCC)
  )

  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CD1AC21)
    (at 69.85 55.92 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (path /5CD25D56)
    (fp_text reference C1 (at 1.25 -2.05 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 2.05 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CE3F180)
    (at 27.9 40.64 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (path /5CD91735)
    (fp_text reference C2 (at 1.25 -2.05 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 2.05 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.25 0 180) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CD1DAF4)
    (at 74.93 66.04 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (path /5CD3F935)
    (fp_text reference C3 (at 1.25 -2.05 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 2.05 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 RESET))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_D8.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CE40C28)
    (at 105.41 38.1 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 8mm Electrolytic Capacitor")
    (path /5CD3C177)
    (fp_text reference C4 (at -5.08 -1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100uF (at 2.5 5.25 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 2.5 0) (end 6.5 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.62 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.5 0) (end 6.75 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.926759 -1.7475) (end -0.126759 -1.7475) (layer F.Fab) (width 0.1))
    (fp_line (start -0.526759 -2.1475) (end -0.526759 -1.3475) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 -4.08) (end 2.5 4.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.54 -4.08) (end 2.54 4.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.58 -4.08) (end 2.58 4.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.62 -4.079) (end 2.62 4.079) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.66 -4.077) (end 2.66 4.077) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.7 -4.076) (end 2.7 4.076) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.74 -4.074) (end 2.74 4.074) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.78 -4.071) (end 2.78 4.071) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.82 -4.068) (end 2.82 4.068) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.86 -4.065) (end 2.86 4.065) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.9 -4.061) (end 2.9 4.061) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.94 -4.057) (end 2.94 4.057) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.98 -4.052) (end 2.98 4.052) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.02 -4.048) (end 3.02 4.048) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.06 -4.042) (end 3.06 4.042) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.1 -4.037) (end 3.1 4.037) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.14 -4.03) (end 3.14 4.03) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.18 -4.024) (end 3.18 4.024) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.221 -4.017) (end 3.221 4.017) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.261 -4.01) (end 3.261 4.01) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.301 -4.002) (end 3.301 4.002) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.341 -3.994) (end 3.341 3.994) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.381 -3.985) (end 3.381 3.985) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.421 -3.976) (end 3.421 3.976) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.461 -3.967) (end 3.461 3.967) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.501 -3.957) (end 3.501 3.957) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.541 -3.947) (end 3.541 3.947) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.581 -3.936) (end 3.581 3.936) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.621 -3.925) (end 3.621 3.925) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.661 -3.914) (end 3.661 3.914) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.701 -3.902) (end 3.701 3.902) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.741 -3.889) (end 3.741 3.889) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.781 -3.877) (end 3.781 3.877) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.821 -3.863) (end 3.821 3.863) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.861 -3.85) (end 3.861 3.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.901 -3.835) (end 3.901 3.835) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.941 -3.821) (end 3.941 3.821) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.981 -3.805) (end 3.981 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.981 1.04) (end 3.981 3.805) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.021 -3.79) (end 4.021 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.021 1.04) (end 4.021 3.79) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.061 -3.774) (end 4.061 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.061 1.04) (end 4.061 3.774) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.101 -3.757) (end 4.101 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.101 1.04) (end 4.101 3.757) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.141 -3.74) (end 4.141 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.141 1.04) (end 4.141 3.74) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.181 -3.722) (end 4.181 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.181 1.04) (end 4.181 3.722) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.221 -3.704) (end 4.221 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.221 1.04) (end 4.221 3.704) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.261 -3.686) (end 4.261 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.261 1.04) (end 4.261 3.686) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.301 -3.666) (end 4.301 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.301 1.04) (end 4.301 3.666) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.341 -3.647) (end 4.341 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.341 1.04) (end 4.341 3.647) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.381 -3.627) (end 4.381 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.381 1.04) (end 4.381 3.627) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.421 -3.606) (end 4.421 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.421 1.04) (end 4.421 3.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.461 -3.584) (end 4.461 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.461 1.04) (end 4.461 3.584) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.501 -3.562) (end 4.501 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.501 1.04) (end 4.501 3.562) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.541 -3.54) (end 4.541 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.541 1.04) (end 4.541 3.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.581 -3.517) (end 4.581 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.581 1.04) (end 4.581 3.517) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.621 -3.493) (end 4.621 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.621 1.04) (end 4.621 3.493) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.661 -3.469) (end 4.661 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.661 1.04) (end 4.661 3.469) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.701 -3.444) (end 4.701 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.701 1.04) (end 4.701 3.444) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.741 -3.418) (end 4.741 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.741 1.04) (end 4.741 3.418) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.781 -3.392) (end 4.781 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.781 1.04) (end 4.781 3.392) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.821 -3.365) (end 4.821 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.821 1.04) (end 4.821 3.365) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.861 -3.338) (end 4.861 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.861 1.04) (end 4.861 3.338) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.901 -3.309) (end 4.901 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.901 1.04) (end 4.901 3.309) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.941 -3.28) (end 4.941 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.941 1.04) (end 4.941 3.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.981 -3.25) (end 4.981 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.981 1.04) (end 4.981 3.25) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.021 -3.22) (end 5.021 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.021 1.04) (end 5.021 3.22) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.061 -3.189) (end 5.061 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.061 1.04) (end 5.061 3.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.101 -3.156) (end 5.101 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.101 1.04) (end 5.101 3.156) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.141 -3.124) (end 5.141 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.141 1.04) (end 5.141 3.124) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.181 -3.09) (end 5.181 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.181 1.04) (end 5.181 3.09) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.221 -3.055) (end 5.221 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.221 1.04) (end 5.221 3.055) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.261 -3.019) (end 5.261 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.261 1.04) (end 5.261 3.019) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.301 -2.983) (end 5.301 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.301 1.04) (end 5.301 2.983) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.341 -2.945) (end 5.341 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.341 1.04) (end 5.341 2.945) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.381 -2.907) (end 5.381 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.381 1.04) (end 5.381 2.907) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.421 -2.867) (end 5.421 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.421 1.04) (end 5.421 2.867) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.461 -2.826) (end 5.461 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.461 1.04) (end 5.461 2.826) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.501 -2.784) (end 5.501 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.501 1.04) (end 5.501 2.784) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.541 -2.741) (end 5.541 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.541 1.04) (end 5.541 2.741) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.581 -2.697) (end 5.581 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.581 1.04) (end 5.581 2.697) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.621 -2.651) (end 5.621 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.621 1.04) (end 5.621 2.651) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.661 -2.604) (end 5.661 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.661 1.04) (end 5.661 2.604) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.701 -2.556) (end 5.701 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.701 1.04) (end 5.701 2.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.741 -2.505) (end 5.741 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.741 1.04) (end 5.741 2.505) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.781 -2.454) (end 5.781 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.781 1.04) (end 5.781 2.454) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.821 -2.4) (end 5.821 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.821 1.04) (end 5.821 2.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.861 -2.345) (end 5.861 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.861 1.04) (end 5.861 2.345) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.901 -2.287) (end 5.901 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.901 1.04) (end 5.901 2.287) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.941 -2.228) (end 5.941 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.941 1.04) (end 5.941 2.228) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.981 -2.166) (end 5.981 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.981 1.04) (end 5.981 2.166) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.021 -2.102) (end 6.021 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.021 1.04) (end 6.021 2.102) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.061 -2.034) (end 6.061 2.034) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.101 -1.964) (end 6.101 1.964) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.141 -1.89) (end 6.141 1.89) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.181 -1.813) (end 6.181 1.813) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.221 -1.731) (end 6.221 1.731) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.261 -1.645) (end 6.261 1.645) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.301 -1.552) (end 6.301 1.552) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.341 -1.453) (end 6.341 1.453) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.381 -1.346) (end 6.381 1.346) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.421 -1.229) (end 6.421 1.229) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.461 -1.098) (end 6.461 1.098) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.501 -0.948) (end 6.501 0.948) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.541 -0.768) (end 6.541 0.768) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.581 -0.533) (end 6.581 0.533) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.909698 -2.315) (end -1.109698 -2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.509698 -2.715) (end -1.509698 -1.915) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CD1DE2A)
    (at 78.74 57.11 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (path /5CD16AB1)
    (fp_text reference C5 (at 1.25 -2.05 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22p (at 1.25 2.05 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CD1AD0E)
    (at 78.74 48.3 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (path /5CD16B2E)
    (fp_text reference C6 (at -2.58 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22p (at 1.25 2.05 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.25 0 270) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_D8.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CD1A962)
    (at 39.37 20.32 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 8mm Electrolytic Capacitor")
    (path /5CDA1999)
    (fp_text reference C7 (at -2.54 -3.81 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470uF (at 2.5 5.25 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.509698 -2.715) (end -1.509698 -1.915) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.909698 -2.315) (end -1.109698 -2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.581 -0.533) (end 6.581 0.533) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.541 -0.768) (end 6.541 0.768) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.501 -0.948) (end 6.501 0.948) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.461 -1.098) (end 6.461 1.098) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.421 -1.229) (end 6.421 1.229) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.381 -1.346) (end 6.381 1.346) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.341 -1.453) (end 6.341 1.453) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.301 -1.552) (end 6.301 1.552) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.261 -1.645) (end 6.261 1.645) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.221 -1.731) (end 6.221 1.731) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.181 -1.813) (end 6.181 1.813) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.141 -1.89) (end 6.141 1.89) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.101 -1.964) (end 6.101 1.964) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.061 -2.034) (end 6.061 2.034) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.021 1.04) (end 6.021 2.102) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.021 -2.102) (end 6.021 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.981 1.04) (end 5.981 2.166) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.981 -2.166) (end 5.981 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.941 1.04) (end 5.941 2.228) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.941 -2.228) (end 5.941 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.901 1.04) (end 5.901 2.287) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.901 -2.287) (end 5.901 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.861 1.04) (end 5.861 2.345) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.861 -2.345) (end 5.861 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.821 1.04) (end 5.821 2.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.821 -2.4) (end 5.821 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.781 1.04) (end 5.781 2.454) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.781 -2.454) (end 5.781 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.741 1.04) (end 5.741 2.505) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.741 -2.505) (end 5.741 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.701 1.04) (end 5.701 2.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.701 -2.556) (end 5.701 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.661 1.04) (end 5.661 2.604) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.661 -2.604) (end 5.661 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.621 1.04) (end 5.621 2.651) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.621 -2.651) (end 5.621 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.581 1.04) (end 5.581 2.697) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.581 -2.697) (end 5.581 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.541 1.04) (end 5.541 2.741) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.541 -2.741) (end 5.541 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.501 1.04) (end 5.501 2.784) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.501 -2.784) (end 5.501 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.461 1.04) (end 5.461 2.826) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.461 -2.826) (end 5.461 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.421 1.04) (end 5.421 2.867) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.421 -2.867) (end 5.421 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.381 1.04) (end 5.381 2.907) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.381 -2.907) (end 5.381 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.341 1.04) (end 5.341 2.945) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.341 -2.945) (end 5.341 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.301 1.04) (end 5.301 2.983) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.301 -2.983) (end 5.301 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.261 1.04) (end 5.261 3.019) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.261 -3.019) (end 5.261 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.221 1.04) (end 5.221 3.055) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.221 -3.055) (end 5.221 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.181 1.04) (end 5.181 3.09) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.181 -3.09) (end 5.181 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.141 1.04) (end 5.141 3.124) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.141 -3.124) (end 5.141 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.101 1.04) (end 5.101 3.156) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.101 -3.156) (end 5.101 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.061 1.04) (end 5.061 3.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.061 -3.189) (end 5.061 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.021 1.04) (end 5.021 3.22) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.021 -3.22) (end 5.021 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.981 1.04) (end 4.981 3.25) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.981 -3.25) (end 4.981 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.941 1.04) (end 4.941 3.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.941 -3.28) (end 4.941 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.901 1.04) (end 4.901 3.309) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.901 -3.309) (end 4.901 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.861 1.04) (end 4.861 3.338) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.861 -3.338) (end 4.861 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.821 1.04) (end 4.821 3.365) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.821 -3.365) (end 4.821 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.781 1.04) (end 4.781 3.392) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.781 -3.392) (end 4.781 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.741 1.04) (end 4.741 3.418) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.741 -3.418) (end 4.741 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.701 1.04) (end 4.701 3.444) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.701 -3.444) (end 4.701 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.661 1.04) (end 4.661 3.469) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.661 -3.469) (end 4.661 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.621 1.04) (end 4.621 3.493) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.621 -3.493) (end 4.621 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.581 1.04) (end 4.581 3.517) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.581 -3.517) (end 4.581 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.541 1.04) (end 4.541 3.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.541 -3.54) (end 4.541 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.501 1.04) (end 4.501 3.562) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.501 -3.562) (end 4.501 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.461 1.04) (end 4.461 3.584) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.461 -3.584) (end 4.461 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.421 1.04) (end 4.421 3.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.421 -3.606) (end 4.421 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.381 1.04) (end 4.381 3.627) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.381 -3.627) (end 4.381 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.341 1.04) (end 4.341 3.647) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.341 -3.647) (end 4.341 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.301 1.04) (end 4.301 3.666) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.301 -3.666) (end 4.301 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.261 1.04) (end 4.261 3.686) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.261 -3.686) (end 4.261 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.221 1.04) (end 4.221 3.704) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.221 -3.704) (end 4.221 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.181 1.04) (end 4.181 3.722) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.181 -3.722) (end 4.181 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.141 1.04) (end 4.141 3.74) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.141 -3.74) (end 4.141 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.101 1.04) (end 4.101 3.757) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.101 -3.757) (end 4.101 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.061 1.04) (end 4.061 3.774) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.061 -3.774) (end 4.061 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.021 1.04) (end 4.021 3.79) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.021 -3.79) (end 4.021 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.981 1.04) (end 3.981 3.805) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.981 -3.805) (end 3.981 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.941 -3.821) (end 3.941 3.821) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.901 -3.835) (end 3.901 3.835) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.861 -3.85) (end 3.861 3.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.821 -3.863) (end 3.821 3.863) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.781 -3.877) (end 3.781 3.877) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.741 -3.889) (end 3.741 3.889) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.701 -3.902) (end 3.701 3.902) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.661 -3.914) (end 3.661 3.914) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.621 -3.925) (end 3.621 3.925) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.581 -3.936) (end 3.581 3.936) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.541 -3.947) (end 3.541 3.947) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.501 -3.957) (end 3.501 3.957) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.461 -3.967) (end 3.461 3.967) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.421 -3.976) (end 3.421 3.976) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.381 -3.985) (end 3.381 3.985) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.341 -3.994) (end 3.341 3.994) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.301 -4.002) (end 3.301 4.002) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.261 -4.01) (end 3.261 4.01) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.221 -4.017) (end 3.221 4.017) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.18 -4.024) (end 3.18 4.024) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.14 -4.03) (end 3.14 4.03) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.1 -4.037) (end 3.1 4.037) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.06 -4.042) (end 3.06 4.042) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.02 -4.048) (end 3.02 4.048) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.98 -4.052) (end 2.98 4.052) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.94 -4.057) (end 2.94 4.057) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.9 -4.061) (end 2.9 4.061) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.86 -4.065) (end 2.86 4.065) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.82 -4.068) (end 2.82 4.068) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.78 -4.071) (end 2.78 4.071) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.74 -4.074) (end 2.74 4.074) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.7 -4.076) (end 2.7 4.076) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.66 -4.077) (end 2.66 4.077) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.62 -4.079) (end 2.62 4.079) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.58 -4.08) (end 2.58 4.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.54 -4.08) (end 2.54 4.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.5 -4.08) (end 2.5 4.08) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.526759 -2.1475) (end -0.526759 -1.3475) (layer F.Fab) (width 0.1))
    (fp_line (start -0.926759 -1.7475) (end -0.126759 -1.7475) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.75 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.5 0) (end 6.62 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.5 0) (end 6.5 0) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 GNDPWR))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CE425C1)
    (at 85.09 68.58 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (path /5CD250AE)
    (fp_text reference C8 (at 1.25 -2.05 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 2.05 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.25 0 270) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CE426C6)
    (at 81.28 48.22 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (path /5CD239F2)
    (fp_text reference C9 (at -2.58 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 1.25 2.05 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CD1D96C)
    (at 82.55 80.01 270)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (path /5CD43722)
    (fp_text reference J3 (at 0 -2.33 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Serial (at 0 15.03 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 13.97) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 13.97) (end -1.27 13.97) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 13.97) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 14.03) (end 1.33 14.03) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 14.03) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 14.03) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 14.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 14.5) (end 1.8 14.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 14.5) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 6.35) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 RESET))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 TX))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 RX))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CD1AE3F)
    (at 54.61 63.5)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (path /5CE19110)
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_Encoder (at 0 9.95) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 9.4) (end 1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 ENCODER_B))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 ENCODER_A))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 ENCODER_BUTTON))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CD1AE55)
    (at 59.69 34.29 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (path /5CD323EC)
    (fp_text reference J5 (at 0 -2.33 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_Motor (at 0 4.87 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 1.27) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CD1AE82)
    (at 49.53 63.5 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (path /5CE08F51)
    (fp_text reference J7 (at 0 -2.33 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_Servo_Poti (at 0 7.41 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 6.35) (end -1.27 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 6.35) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 6.41) (end 1.33 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 6.85) (end 1.8 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 6.85) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 SERVO_SLIDER))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Jumper:SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm (layer F.Cu) (tedit 5D514AAE) (tstamp 5CD1AECA)
    (at 69.23 27.94 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (path /5CDBB9F4)
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8 180) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SolderJumper_5V_VCC (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 1) (end -1.4 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 1) (end -1.4 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 -1) (end 1.4 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -1) (end 1.4 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.65 -1.25) (end 1.65 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.65 -1.25) (end -1.65 1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.25) (end 1.65 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.65 1.25) (end -1.65 1.25) (layer F.CrtYd) (width 0.05))
    (pad 1 smd custom (at -0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 2 +5V)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.4 -0.3) (xy 0.9 -0.3) (xy 0.9 0.3) (xy 0.4 0.3)) (width 0))
      ))
    (pad 2 smd rect (at 0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 7 VCC))
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CD1AEFE)
    (at 74.93 73.66 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5CD153B9)
    (fp_text reference R2 (at -1.27 2.54 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 2.54 1.92 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.74 -0.8) (end 0.74 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0.74 0.8) (end 4.34 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 4.34 0.8) (end 4.34 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 4.34 -0.8) (end 0.74 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.74 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.08 0) (end 4.34 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.62 -0.92) (end 4.46 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.62 0.92) (end 4.46 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 6.03 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.03 1.05) (end 6.03 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.03 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.54 0 180) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-28_W7.62mm (layer F.Cu) (tedit 5A02E8C5) (tstamp 5CD1AF41)
    (at 67.31 73.66 180)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (path /5CD141F3)
    (fp_text reference U1 (at 3.81 -2.33 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ATmega328P-PU (at 3.81 35.35 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 34.29) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 34.29) (end 0.635 34.29) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 34.29) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 34.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 34.35) (end 6.46 34.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 34.35) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.55) (end -1.1 34.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 34.55) (end 8.7 34.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 34.55) (end 8.7 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 16.51 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 33.02 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(J9-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 RX))
    (pad 16 thru_hole oval (at 7.62 30.48 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 SS))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 TX))
    (pad 17 thru_hole oval (at 7.62 27.94 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 MOSI))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 SRDATA))
    (pad 18 thru_hole oval (at 7.62 25.4 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 MISO))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 SRCLOCK))
    (pad 19 thru_hole oval (at 7.62 22.86 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 SCK))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 SRLATCH))
    (pad 20 thru_hole oval (at 7.62 20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 21 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 22 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (pad 23 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 SERVO_SLIDER))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (pad 24 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 ENCODER_B))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 MOTOR_1))
    (pad 25 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 ENCODER_A))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 MOTOR_2))
    (pad 26 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 ENCODER_BUTTON))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 28 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157) (tstamp 5CE3F1F0)
    (at 22.86 35.56 270)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (path /5CD8B474)
    (fp_text reference U2 (at 1.27 -3.56 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value L78L33_TO92 (at 1.27 2.79 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.27 -3.56 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 1.75) (end 3 1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1.46 -2.73) (end 4 -2.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4 2.01) (end 4 -2.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4 2.01) (end -1.46 2.01) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 1.27 0) (end 1.27 -2.48) (angle 135) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.27 0) (end 1.27 -2.6) (angle -135) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 1.27 -2.48) (angle -135) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.27 0) (end 1.27 -2.6) (angle 135) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 12 /3v3))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5) (tstamp 5CD1AF77)
    (at 46.99 27.94 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (path /5CD2818F)
    (fp_text reference U3 (at 5.08 21.59 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value L293D (at 3.81 20.11 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 19.05) (end 0.635 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 19.05) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 19.11) (end 6.46 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 19.11) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.55) (end -1.1 19.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 19.3) (end 8.7 19.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 19.3) (end 8.7 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 MOTOR_1))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J5-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 GNDPWR))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 GNDPWR))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 GNDPWR))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 GNDPWR))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J5-Pad1)"))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 MOTOR_2))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 VCC))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5) (tstamp 5CE42820)
    (at 96.52 35.56 270)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (path /5CD17EBC)
    (fp_text reference U4 (at 3.81 -2.33 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 74HC595 (at 3.81 20.11 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 19.05) (end 0.635 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 19.05) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 19.11) (end 6.46 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 19.11) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.55) (end -1.1 19.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 19.3) (end 8.7 19.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 19.3) (end 8.7 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 8.89 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U4-Pad1)"))
    (pad 9 thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(U4-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(U4-Pad3)"))
    (pad 11 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 SRCLOCK))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(U4-Pad4)"))
    (pad 12 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 SRLATCH))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(U4-Pad5)"))
    (pad 13 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(U4-Pad6)"))
    (pad 14 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(U4-Pad14)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(U4-Pad7)"))
    (pad 15 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U4-Pad15)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 16 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5) (tstamp 5CE42748)
    (at 95.25 71.12 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (path /5CD1CCAE)
    (fp_text reference U5 (at 3.81 -2.33 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 74HC595 (at 3.81 20.11 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 8.89 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 19.3) (end 8.7 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 19.3) (end 8.7 19.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 -1.55) (end -1.1 19.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 19.11) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 19.11) (end 6.46 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 19.05) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 19.05) (end 0.635 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U5-Pad15)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(U5-Pad7)"))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 SRDATA))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(U5-Pad6)"))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(U5-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 SRLATCH))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(U5-Pad4)"))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 SRCLOCK))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(U5-Pad3)"))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(U5-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(U4-Pad14)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(U5-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-18_W7.62mm (layer F.Cu) (tedit 5A02E8C5) (tstamp 5CE4266C)
    (at 81.28 30.48 90)
    (descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (path /5CE689B3)
    (fp_text reference U6 (at 3.81 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ULN2803A (at 3.81 22.65 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 21.59) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 21.59) (end 0.635 21.59) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 21.59) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 21.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 21.65) (end 6.46 21.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 21.65) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.55) (end -1.1 21.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 21.85) (end 8.7 21.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 21.85) (end 8.7 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 10.16 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(U4-Pad7)"))
    (pad 10 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +9V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(U4-Pad6)"))
    (pad 11 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J8-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(U4-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J8-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(U4-Pad4)"))
    (pad 13 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J8-Pad3)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(U4-Pad3)"))
    (pad 14 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(J8-Pad4)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(U4-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(J8-Pad5)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U4-Pad1)"))
    (pad 16 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(J8-Pad6)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U4-Pad15)"))
    (pad 17 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(J8-Pad7)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 GNDPWR))
    (pad 18 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(J8-Pad8)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-18_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-18_W7.62mm (layer F.Cu) (tedit 5A02E8C5) (tstamp 5CE427B3)
    (at 100.33 55.88)
    (descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (path /5CDD2737)
    (fp_text reference U7 (at 3.81 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ULN2803A (at 3.81 22.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 10.16) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 21.85) (end 8.7 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 21.85) (end 8.7 21.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 -1.55) (end -1.1 21.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 21.65) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 21.65) (end 6.46 21.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 21.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 21.59) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 21.59) (end 0.635 21.59) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 21.59) (layer F.Fab) (width 0.1))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (pad 18 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(J6-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 GNDPWR))
    (pad 17 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(J6-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U5-Pad15)"))
    (pad 16 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(J6-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(U5-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(J6-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(U5-Pad2)"))
    (pad 14 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(J6-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(U5-Pad3)"))
    (pad 13 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(J6-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(U5-Pad4)"))
    (pad 12 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(J6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(U5-Pad5)"))
    (pad 11 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(J6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(U5-Pad6)"))
    (pad 10 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +9V))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(U5-Pad7)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-18_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Crystal:Crystal_HC52-6mm_Vertical (layer F.Cu) (tedit 5A1AD3B8) (tstamp 5CD1B022)
    (at 74.93 54.6 90)
    (descr "Crystal THT HC-52/6mm, http://www.kvg-gmbh.de/assets/uploads/files/product_pdfs/XS71xx.pdf")
    (tags "THT crystalHC-49/U")
    (path /5CD163A1)
    (fp_text reference Y1 (at 1.9 -2.85 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Crystal (at 1.9 2.85 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.9 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.45 -1.65) (end 4.25 -1.65) (layer F.Fab) (width 0.1))
    (fp_line (start -0.45 1.65) (end 4.25 1.65) (layer F.Fab) (width 0.1))
    (fp_line (start -0.45 -1.15) (end 4.25 -1.15) (layer F.Fab) (width 0.1))
    (fp_line (start -0.45 1.15) (end 4.25 1.15) (layer F.Fab) (width 0.1))
    (fp_line (start -0.45 -1.85) (end 4.25 -1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.45 1.85) (end 4.25 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -2.1) (end -2.6 2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 2.1) (end 6.4 2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.4 2.1) (end 6.4 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.4 -2.1) (end -2.6 -2.1) (layer F.CrtYd) (width 0.05))
    (fp_arc (start -0.45 0) (end -0.45 -1.65) (angle -180) (layer F.Fab) (width 0.1))
    (fp_arc (start 4.25 0) (end 4.25 -1.65) (angle 180) (layer F.Fab) (width 0.1))
    (fp_arc (start -0.45 0) (end -0.45 -1.15) (angle -180) (layer F.Fab) (width 0.1))
    (fp_arc (start 4.25 0) (end 4.25 -1.15) (angle 180) (layer F.Fab) (width 0.1))
    (fp_arc (start -0.45 0) (end -0.45 -1.85) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_arc (start 4.25 0) (end 4.25 -1.85) (angle 180) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (pad 2 thru_hole circle (at 3.8 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_HC52-6mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:W5100_V2 (layer F.Cu) (tedit 5CD1A29F) (tstamp 5CE3F1B5)
    (at 31.75 32.385 270)
    (path /5CD7CCFC)
    (fp_text reference J1 (at 5.835 -6.71 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_w5100 (at 5.835 -7.71 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 33 -8) (end 54 -8) (layer F.SilkS) (width 0.15))
    (fp_line (start 33 8) (end 33 -8) (layer F.SilkS) (width 0.15))
    (fp_line (start 54 8) (end 33 8) (layer F.SilkS) (width 0.15))
    (fp_line (start 54 -8) (end 54 8) (layer F.SilkS) (width 0.15))
    (fp_line (start 50 14) (end 0 14) (layer F.SilkS) (width 0.15))
    (fp_line (start 50 -14) (end 50 14) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -14) (end 50 -14) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 14) (end 0 -14) (layer F.SilkS) (width 0.15))
    (pad "" np_thru_hole circle (at 47.5 11.25 270) (size 3 3) (drill 2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 47.5 -11.25 270) (size 3 3) (drill 2) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 1.905 3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 /3v3))
    (pad 7 thru_hole circle (at 1.905 1.27 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 MISO))
    (pad 6 thru_hole circle (at 1.905 -1.27 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 SS))
    (pad 5 thru_hole circle (at 1.905 -3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 4.445 -3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 4.445 -1.27 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 SCK))
    (pad 2 thru_hole circle (at 4.445 1.27 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 MOSI))
    (pad 1 thru_hole circle (at 4.445 3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GNDD))
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CE40D90)
    (at 113.03 33.02)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (path /5CD2E3E6)
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_5V_9V (at 0 12.49) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 11.43) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 11.43) (end -1.27 11.43) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 11.43) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 11.49) (end 1.33 11.49) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 11.49) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 11.49) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 11.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 11.95) (end 1.8 11.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 11.95) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 +9V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Jumper:SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm (layer B.Cu) (tedit 5D514AB3) (tstamp 5CD1B15F)
    (at 71.755 32.385 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (path /5CDC4DD2)
    (attr virtual)
    (fp_text reference JP2 (at 0 1.8 90) (layer B.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value SolderJumper_5V_VCC (at 0 -1.905 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -1.4 -1) (end -1.4 1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.4 -1) (end -1.4 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.4 1) (end 1.4 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 1) (end 1.4 1) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.65 1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (pad 1 smd custom (at -0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 1 GNDD)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.4 0.3) (xy 0.9 0.3) (xy 0.9 -0.3) (xy 0.4 -0.3)) (width 0))
      ))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 59 GNDPWR))
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CE42601)
    (at 113.03 73.66 180)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (path /5CE493D3)
    (fp_text reference J6 (at 0 -2.33 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_relayB (at 0 25.19 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 24.13) (end -1.27 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 24.13) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 24.19) (end 1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 24.65) (end 1.8 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 24.65) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 11.43 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(J6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(J6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(J6-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(J6-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(J6-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(J6-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(J6-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J6-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 +9V))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 +9V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CE4289B)
    (at 99.06 17.78 270)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (path /5CE53F87)
    (fp_text reference J8 (at 0 -2.33 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_relayA (at 0 25.19 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 11.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 24.65) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 24.65) (end 1.8 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 24.19) (end 1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 24.13) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 24.13) (end -1.27 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 +9V))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 +9V))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J8-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J8-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J8-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J8-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J8-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J8-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J8-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J8-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5D51556A)
    (at 48.26 40.64 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (path /5D524EBB)
    (fp_text reference J9 (at 3.175 -1.27 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_WS2812 (at 0 7.41 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 6.35) (end -1.27 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 6.35) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 6.41) (end 1.33 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 6.85) (end 1.8 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 6.85) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(J9-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text LED (at 50.165 37.465) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "GND 5V S" (at 50.165 43.18) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.25)))
  )
  (gr_text Motor (at 58.42 31.75) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "GND 5V 9V" (at 110.49 38.1 90) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "9V  8 7 6 5 4 3 2 1" (at 109.855 49.53 270) (layer F.SilkS) (tstamp 5D515309)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify left))
  )
  (gr_text "9V  8 7 6 5 4 3 2 1" (at 75.565 20.955) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify left))
  )
  (gr_text | (at 113.03 78.105) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Relay B" (at 111.76 80.645) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Relay A" (at 69.215 17.78) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "G S A B" (at 57.15 67.31 90) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "G S 5V" (at 46.99 60.325 90) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text Encoder (at 54.61 57.15 90) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text VolServo (at 49.53 50.8 90) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "GND    5V RX TX RST" (at 67.945 76.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.25)) (justify left))
  )
  (gr_line (start 12.7 82.7) (end 12.7 12.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.84 82.7) (end 12.7 82.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.84 12.7) (end 116.84 82.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 12.7 12.7) (end 116.84 12.7) (layer Edge.Cuts) (width 0.15))

  (via (at 17.145 17.145) (size 5) (drill 3.1) (layers F.Cu B.Cu) (net 0))
  (via (at 112.145 17.145) (size 5) (drill 3.1) (layers F.Cu B.Cu) (net 0) (tstamp 5CE44F95))
  (via (at 92.145 79.145) (size 5) (drill 3.1) (layers F.Cu B.Cu) (net 0) (tstamp 5CE44FA0))
  (via (at 17.145 67.145) (size 5) (drill 3.1) (layers F.Cu B.Cu) (net 0) (tstamp 5CE44FA4))
  (via (at 52.07 78.74) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 1))
  (segment (start 69.81 55.88) (end 69.85 55.92) (width 1) (layer B.Cu) (net 1) (status 30))
  (segment (start 67.31 55.88) (end 69.81 55.88) (width 1) (layer B.Cu) (net 1) (status 30))
  (segment (start 69.85 55.92) (end 70.98137 55.92) (width 1) (layer B.Cu) (net 1) (status 10))
  (segment (start 79.87137 48.3) (end 81.28 49.70863) (width 1) (layer B.Cu) (net 1))
  (segment (start 78.74 48.3) (end 79.87137 48.3) (width 1) (layer B.Cu) (net 1) (status 10))
  (segment (start 79.87137 57.11) (end 78.74 57.11) (width 1) (layer B.Cu) (net 1) (status 20))
  (segment (start 81.28 55.70137) (end 79.87137 57.11) (width 1) (layer B.Cu) (net 1))
  (segment (start 81.28 49.70863) (end 81.28 55.70137) (width 1) (layer B.Cu) (net 1))
  (segment (start 53.407919 71.12) (end 54.61 71.12) (width 1) (layer B.Cu) (net 1) (status 20))
  (segment (start 49.53 67.242081) (end 53.407919 71.12) (width 1) (layer B.Cu) (net 1))
  (segment (start 49.53 63.5) (end 49.53 67.242081) (width 1) (layer B.Cu) (net 1) (status 10))
  (segment (start 27.94 36.83) (end 22.86 36.83) (width 1) (layer B.Cu) (net 1) (status 30))
  (segment (start 27.9 36.87) (end 27.94 36.83) (width 1) (layer B.Cu) (net 1) (status 30))
  (segment (start 27.9 40.64) (end 27.9 36.87) (width 1) (layer B.Cu) (net 1) (status 30))
  (segment (start 105.49 43.18) (end 105.41 43.1) (width 1) (layer B.Cu) (net 1) (status 30))
  (segment (start 113.03 43.18) (end 105.49 43.18) (width 1.5) (layer B.Cu) (net 1) (status 30))
  (segment (start 113.03 40.64) (end 113.03 43.18) (width 1) (layer B.Cu) (net 1) (status 30))
  (segment (start 59.69 58.42) (end 62.23 58.42) (width 1) (layer B.Cu) (net 1) (status 10))
  (segment (start 62.23 58.42) (end 64.77 55.88) (width 1) (layer B.Cu) (net 1))
  (segment (start 64.77 55.88) (end 67.31 55.88) (width 1) (layer B.Cu) (net 1) (status 20))
  (segment (start 95.25 53.26) (end 95.25 53.34) (width 1) (layer B.Cu) (net 1) (status 30))
  (segment (start 88.9 43.18) (end 88.9 46.99) (width 1.5) (layer F.Cu) (net 1) (status 10))
  (segment (start 99.06 46.99) (end 95.25 46.99) (width 1.5) (layer B.Cu) (net 1))
  (segment (start 95.25 46.99) (end 95.25 53.34) (width 1.5) (layer B.Cu) (net 1) (status 20))
  (via (at 95.25 46.99) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 1))
  (segment (start 95.25 46.99) (end 88.9 46.99) (width 1.5) (layer F.Cu) (net 1))
  (segment (start 87.63 63.5) (end 88.9 63.5) (width 1) (layer B.Cu) (net 1) (status 10))
  (segment (start 88.9 63.5) (end 91.44 60.96) (width 1) (layer B.Cu) (net 1))
  (segment (start 91.44 60.96) (end 91.44 54.61) (width 1) (layer B.Cu) (net 1))
  (segment (start 91.44 54.61) (end 92.71 53.34) (width 1) (layer B.Cu) (net 1))
  (segment (start 92.71 53.34) (end 95.25 53.34) (width 1) (layer B.Cu) (net 1) (status 20))
  (segment (start 72.17137 57.11) (end 70.98137 55.92) (width 1) (layer B.Cu) (net 1))
  (segment (start 78.74 57.11) (end 72.17137 57.11) (width 1) (layer B.Cu) (net 1) (status 10))
  (segment (start 85.09 68.58) (end 85.09 64.77) (width 1) (layer F.Cu) (net 1) (status 10))
  (segment (start 85.09 64.77) (end 86.36 63.5) (width 1) (layer F.Cu) (net 1))
  (segment (start 86.36 63.5) (end 87.63 63.5) (width 2) (layer F.Cu) (net 1) (status 20))
  (segment (start 27.9 41.77137) (end 27.9 40.64) (width 1) (layer F.Cu) (net 1) (status 20))
  (segment (start 27.9 43.72) (end 27.9 41.77137) (width 1) (layer F.Cu) (net 1))
  (segment (start 47.68 63.5) (end 27.9 43.72) (width 1) (layer F.Cu) (net 1))
  (segment (start 49.53 63.5) (end 47.68 63.5) (width 1) (layer F.Cu) (net 1) (status 10))
  (segment (start 51.38 63.5) (end 52.07 62.81) (width 1) (layer F.Cu) (net 1))
  (segment (start 49.53 63.5) (end 51.38 63.5) (width 1) (layer F.Cu) (net 1) (status 10))
  (segment (start 52.07 62.81) (end 52.07 60.96) (width 1) (layer F.Cu) (net 1))
  (segment (start 54.61 58.42) (end 59.69 58.42) (width 1) (layer F.Cu) (net 1) (status 20))
  (segment (start 52.07 60.96) (end 54.61 58.42) (width 1) (layer F.Cu) (net 1))
  (segment (start 78.74 38.1) (end 78.74 35.56) (width 1) (layer B.Cu) (net 1) (status 20))
  (segment (start 88.9 43.18) (end 88.9 41.91) (width 1) (layer B.Cu) (net 1) (status 10))
  (segment (start 86.36 39.37) (end 80.01 39.37) (width 1) (layer B.Cu) (net 1))
  (segment (start 80.01 39.37) (end 78.74 38.1) (width 1) (layer B.Cu) (net 1))
  (segment (start 88.9 41.91) (end 86.36 39.37) (width 1) (layer B.Cu) (net 1))
  (segment (start 80.01 39.37) (end 77.47 39.37) (width 1) (layer B.Cu) (net 1))
  (segment (start 77.47 39.37) (end 74.93 41.91) (width 1) (layer B.Cu) (net 1))
  (segment (start 74.93 44.49) (end 78.74 48.3) (width 1) (layer B.Cu) (net 1) (status 20))
  (segment (start 74.93 41.91) (end 74.93 44.49) (width 1) (layer B.Cu) (net 1))
  (segment (start 62.23 71.620002) (end 62.23 71.12) (width 1) (layer B.Cu) (net 1))
  (segment (start 62.23 71.12) (end 62.23 58.42) (width 1) (layer B.Cu) (net 1))
  (via (at 25.4 26.67) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 1) (tstamp 5CE451B6))
  (via (at 86.36 74.93) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 1) (tstamp 5CE451B8))
  (via (at 71.755 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 1) (tstamp 5CE451BC))
  (via (at 26.67 78.74) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 1) (tstamp 5CE454DC))
  (via (at 36.83 78.74) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 1) (tstamp 5CE454DE))
  (via (at 36.83 69.85) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 1) (tstamp 5CE454E0))
  (via (at 26.67 69.85) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 1) (tstamp 5CE454E2))
  (segment (start 78.82 48.22) (end 78.74 48.3) (width 1) (layer B.Cu) (net 1))
  (segment (start 81.28 48.22) (end 78.82 48.22) (width 1) (layer B.Cu) (net 1))
  (segment (start 81.28 48.22) (end 81.28 49.70863) (width 1) (layer B.Cu) (net 1))
  (via (at 52.705 53.34) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 1) (tstamp 5CE6743B))
  (segment (start 62.23 76.2) (end 63.5 77.47) (width 1) (layer B.Cu) (net 1))
  (segment (start 62.23 71.12) (end 62.23 76.2) (width 1) (layer B.Cu) (net 1))
  (segment (start 63.5 77.47) (end 69.85 77.47) (width 1) (layer B.Cu) (net 1))
  (segment (start 69.85 77.47) (end 69.85 80.01) (width 1) (layer B.Cu) (net 1))
  (segment (start 86.36 77.47) (end 86.36 74.93) (width 1) (layer B.Cu) (net 1))
  (segment (start 69.85 77.47) (end 86.36 77.47) (width 1) (layer B.Cu) (net 1))
  (segment (start 86.36 74.93) (end 87.63 74.93) (width 1) (layer F.Cu) (net 1))
  (segment (start 87.63 74.93) (end 90.17 72.39) (width 1) (layer F.Cu) (net 1))
  (segment (start 90.17 72.39) (end 90.17 64.77) (width 1) (layer F.Cu) (net 1))
  (segment (start 90.17 64.77) (end 88.9 63.5) (width 1) (layer F.Cu) (net 1))
  (segment (start 88.9 63.5) (end 87.63 63.5) (width 2) (layer F.Cu) (net 1))
  (segment (start 71.755 33.035) (end 71.755 35.56) (width 1) (layer B.Cu) (net 1))
  (segment (start 78.74 38.1) (end 77.47 39.37) (width 1) (layer B.Cu) (net 1))
  (segment (start 74.93 36.83) (end 73.025 36.83) (width 1) (layer B.Cu) (net 1))
  (segment (start 73.025 36.83) (end 71.755 35.56) (width 1) (layer B.Cu) (net 1))
  (segment (start 77.47 39.37) (end 74.93 36.83) (width 1) (layer B.Cu) (net 1))
  (segment (start 101.52 46.99) (end 105.41 43.1) (width 1.5) (layer B.Cu) (net 1))
  (segment (start 99.06 46.99) (end 101.52 46.99) (width 1.5) (layer B.Cu) (net 1))
  (segment (start 80.01 73.66) (end 76.630001 73.66) (width 1) (layer B.Cu) (net 2) (status 10))
  (segment (start 22.86 38.1) (end 25.4 40.64) (width 1) (layer B.Cu) (net 2) (status 30))
  (segment (start 85.13 71.12) (end 85.09 71.08) (width 1) (layer B.Cu) (net 2) (status 30))
  (segment (start 87.63 71.12) (end 85.13 71.12) (width 1) (layer B.Cu) (net 2) (status 30))
  (segment (start 81.28 45.72) (end 81.28 43.18) (width 1.5) (layer B.Cu) (net 2) (status 30))
  (segment (start 82.41137 45.72) (end 83.82 47.12863) (width 1.5) (layer B.Cu) (net 2))
  (segment (start 81.28 45.72) (end 82.41137 45.72) (width 1.5) (layer B.Cu) (net 2) (status 10))
  (segment (start 83.82 47.12863) (end 83.82 54.61) (width 1.5) (layer B.Cu) (net 2))
  (segment (start 85.09 55.88) (end 87.63 55.88) (width 1.5) (layer B.Cu) (net 2) (status 20))
  (segment (start 83.82 54.61) (end 85.09 55.88) (width 1.5) (layer B.Cu) (net 2))
  (segment (start 113.03 38.1) (end 105.41 38.1) (width 2) (layer B.Cu) (net 2) (status 30))
  (segment (start 96.52 43.18) (end 99.06 43.18) (width 2) (layer B.Cu) (net 2) (status 10))
  (segment (start 99.06 43.18) (end 104.14 38.1) (width 2) (layer B.Cu) (net 2))
  (segment (start 104.14 38.1) (end 105.41 38.1) (width 2) (layer B.Cu) (net 2) (status 20))
  (segment (start 113.03 35.56) (end 113.03 38.1) (width 1) (layer B.Cu) (net 2) (status 30))
  (segment (start 59.69 53.34) (end 59.69 55.88) (width 1) (layer B.Cu) (net 2) (status 30))
  (segment (start 67.31 58.42) (end 64.77 58.42) (width 1.5) (layer F.Cu) (net 2) (status 10))
  (segment (start 62.23 55.88) (end 59.69 55.88) (width 1.5) (layer F.Cu) (net 2) (status 20))
  (segment (start 64.77 58.42) (end 62.23 55.88) (width 1.5) (layer F.Cu) (net 2))
  (segment (start 49.53 58.42) (end 52.07 58.42) (width 1.5) (layer B.Cu) (net 2) (status 10))
  (segment (start 54.61 55.88) (end 59.69 55.88) (width 1.5) (layer B.Cu) (net 2) (status 20))
  (segment (start 52.07 58.42) (end 54.61 55.88) (width 1.5) (layer B.Cu) (net 2))
  (segment (start 67.31 58.42) (end 69.85 58.42) (width 1.5) (layer F.Cu) (net 2) (status 30))
  (segment (start 83.82 55.88) (end 85.09 55.88) (width 1.5) (layer B.Cu) (net 2))
  (segment (start 81.28 58.42) (end 83.82 55.88) (width 1.5) (layer B.Cu) (net 2))
  (segment (start 74.93 73.66) (end 76.630001 73.66) (width 1) (layer B.Cu) (net 2) (status 10))
  (segment (start 82.51 73.66) (end 85.09 71.08) (width 1) (layer B.Cu) (net 2) (status 20))
  (segment (start 80.01 73.66) (end 82.51 73.66) (width 1) (layer B.Cu) (net 2) (status 10))
  (segment (start 81.28 40.64) (end 81.28 43.18) (width 1.5) (layer F.Cu) (net 2) (status 20))
  (segment (start 96.52 41.91) (end 95.25 40.64) (width 1.5) (layer F.Cu) (net 2))
  (segment (start 95.25 40.64) (end 81.28 40.64) (width 1.5) (layer F.Cu) (net 2))
  (segment (start 96.52 43.18) (end 96.52 41.91) (width 1.5) (layer F.Cu) (net 2) (status 10))
  (segment (start 81.28 40.64) (end 76.2 40.64) (width 1.5) (layer F.Cu) (net 2))
  (segment (start 76.2 40.64) (end 74.93 39.37) (width 1.5) (layer F.Cu) (net 2))
  (segment (start 74.93 39.37) (end 74.93 30.48) (width 1) (layer F.Cu) (net 2))
  (segment (start 74.93 30.48) (end 72.39 27.94) (width 1) (layer F.Cu) (net 2))
  (segment (start 72.39 27.94) (end 69.88 27.94) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 80.480001 59.219999) (end 81.28 58.42) (width 1.5) (layer B.Cu) (net 2))
  (segment (start 70.649999 59.219999) (end 80.480001 59.219999) (width 1.5) (layer B.Cu) (net 2))
  (segment (start 69.85 58.42) (end 70.649999 59.219999) (width 1.5) (layer B.Cu) (net 2) (status 10))
  (segment (start 43.18 58.42) (end 29.21 44.45) (width 1.5) (layer B.Cu) (net 2))
  (segment (start 49.53 58.42) (end 43.18 58.42) (width 1.5) (layer B.Cu) (net 2) (status 10))
  (segment (start 29.21 44.45) (end 26.67 44.45) (width 1.5) (layer B.Cu) (net 2))
  (segment (start 26.67 44.45) (end 25.4 43.18) (width 1.5) (layer B.Cu) (net 2))
  (segment (start 25.4 43.18) (end 25.4 40.64) (width 1.5) (layer B.Cu) (net 2) (status 20))
  (segment (start 64.135 59.69) (end 65.405 58.42) (width 1) (layer B.Cu) (net 2))
  (segment (start 65.405 58.42) (end 67.31 58.42) (width 1) (layer B.Cu) (net 2) (status 20))
  (segment (start 74.93 73.66) (end 73.025 75.565) (width 1) (layer B.Cu) (net 2) (status 10))
  (segment (start 73.025 75.565) (end 64.77 75.565) (width 1) (layer B.Cu) (net 2))
  (segment (start 64.77 75.565) (end 64.135 74.93) (width 1) (layer B.Cu) (net 2))
  (segment (start 64.135 74.93) (end 64.135 59.69) (width 1) (layer B.Cu) (net 2))
  (segment (start 74.93 73.66) (end 74.93 80.01) (width 1) (layer F.Cu) (net 2))
  (segment (start 83.82 54.61) (end 83.82 55.88) (width 1.5) (layer B.Cu) (net 2))
  (segment (start 50.8 40.64) (end 50.8 38.1) (width 1.5) (layer B.Cu) (net 2))
  (segment (start 50.8 38.1) (end 52.07 36.83) (width 1.5) (layer B.Cu) (net 2))
  (segment (start 52.07 36.83) (end 66.655998 36.83) (width 1.5) (layer B.Cu) (net 2))
  (segment (start 66.655998 36.83) (end 69.85 36.83) (width 1.5) (layer B.Cu) (net 2))
  (segment (start 69.85 36.83) (end 72.39 39.37) (width 1.5) (layer B.Cu) (net 2))
  (via (at 72.39 39.37) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 72.39 39.37) (end 74.93 39.37) (width 1.5) (layer F.Cu) (net 2))
  (segment (start 74.93 66.04) (end 81.28 66.04) (width 1) (layer F.Cu) (net 3))
  (segment (start 81.28 66.04) (end 82.55 67.31) (width 1) (layer F.Cu) (net 3))
  (segment (start 82.55 67.31) (end 82.55 80.01) (width 1) (layer F.Cu) (net 3))
  (segment (start 67.31 73.66) (end 69.85 73.66) (width 1) (layer B.Cu) (net 4) (status 30))
  (segment (start 72.39 73.66) (end 72.43 73.62) (width 1) (layer B.Cu) (net 4))
  (segment (start 72.43 73.62) (end 72.43 66.04) (width 1) (layer B.Cu) (net 4) (status 20))
  (segment (start 69.85 73.66) (end 72.39 73.66) (width 1) (layer B.Cu) (net 4) (status 10))
  (segment (start 74.93 54.6) (end 73.65 54.6) (width 1) (layer B.Cu) (net 5) (status 10))
  (segment (start 72.39 53.34) (end 67.31 53.34) (width 1) (layer B.Cu) (net 5) (status 20))
  (segment (start 73.65 54.6) (end 72.39 53.34) (width 1) (layer B.Cu) (net 5))
  (segment (start 74.94 54.61) (end 74.93 54.6) (width 1) (layer B.Cu) (net 5) (status 30))
  (segment (start 78.74 54.61) (end 74.94 54.61) (width 1) (layer B.Cu) (net 5) (status 30))
  (segment (start 67.31 50.8) (end 74.93 50.8) (width 1) (layer B.Cu) (net 6) (status 30))
  (segment (start 74.93 50.8) (end 78.74 50.8) (width 1) (layer B.Cu) (net 6) (status 30))
  (segment (start 64.77 27.94) (end 68.17999 27.94) (width 1) (layer F.Cu) (net 7) (status 30))
  (segment (start 39.37 20.32) (end 46.99 20.32) (width 1) (layer B.Cu) (net 7) (status 30))
  (segment (start 64.77 27.94) (end 64.77 25.4) (width 1) (layer F.Cu) (net 7) (status 10))
  (segment (start 64.77 25.4) (end 63.5 24.13) (width 1) (layer F.Cu) (net 7))
  (segment (start 63.5 24.13) (end 48.26 24.13) (width 1) (layer F.Cu) (net 7))
  (segment (start 48.26 24.13) (end 46.99 22.86) (width 1) (layer F.Cu) (net 7))
  (segment (start 46.99 22.86) (end 46.99 20.32) (width 1) (layer F.Cu) (net 7) (status 20))
  (segment (start 39.37 45.72) (end 30.48 36.83) (width 1) (layer B.Cu) (net 8) (status 20))
  (segment (start 59.814002 45.72) (end 59.69 45.72) (width 1) (layer B.Cu) (net 8) (status 30))
  (segment (start 39.37 45.72) (end 59.814002 45.72) (width 1) (layer B.Cu) (net 8) (status 20))
  (segment (start 33.02 41.91) (end 33.02 36.83) (width 1) (layer F.Cu) (net 9) (status 20))
  (segment (start 41.91 50.8) (end 33.02 41.91) (width 1) (layer F.Cu) (net 9))
  (segment (start 59.69 50.8) (end 41.91 50.8) (width 1) (layer F.Cu) (net 9) (status 10))
  (segment (start 33.02 33.02) (end 33.02 34.29) (width 1) (layer B.Cu) (net 10) (status 20))
  (segment (start 34.29 31.75) (end 33.02 33.02) (width 1) (layer B.Cu) (net 10))
  (segment (start 41.91 43.18) (end 39.37 40.64) (width 1) (layer B.Cu) (net 10))
  (segment (start 39.37 40.64) (end 39.37 33.02) (width 1) (layer B.Cu) (net 10))
  (segment (start 38.1 31.75) (end 34.29 31.75) (width 1) (layer B.Cu) (net 10))
  (segment (start 39.37 33.02) (end 38.1 31.75) (width 1) (layer B.Cu) (net 10))
  (segment (start 41.91 43.18) (end 59.69 43.18) (width 1) (layer B.Cu) (net 10) (status 20))
  (segment (start 30.48 33.02) (end 30.48 34.29) (width 1) (layer F.Cu) (net 11) (status 20))
  (segment (start 31.75 31.75) (end 30.48 33.02) (width 1) (layer F.Cu) (net 11))
  (segment (start 38.1 41.91) (end 38.1 33.02) (width 1) (layer F.Cu) (net 11))
  (segment (start 36.83 31.75) (end 31.75 31.75) (width 1) (layer F.Cu) (net 11))
  (segment (start 44.45 48.26) (end 38.1 41.91) (width 1) (layer F.Cu) (net 11))
  (segment (start 38.1 33.02) (end 36.83 31.75) (width 1) (layer F.Cu) (net 11))
  (segment (start 59.814002 48.26) (end 59.69 48.26) (width 1) (layer F.Cu) (net 11) (status 30))
  (segment (start 44.45 48.26) (end 59.814002 48.26) (width 1) (layer F.Cu) (net 11) (status 20))
  (segment (start 24.13 34.29) (end 23.11501 35.30499) (width 1) (layer B.Cu) (net 12) (status 20))
  (segment (start 27.94 34.29) (end 24.13 34.29) (width 1) (layer B.Cu) (net 12) (status 10))
  (segment (start 67.31 68.58) (end 76.2 68.58) (width 1) (layer F.Cu) (net 13))
  (segment (start 80.01 80.01) (end 80.01 71.12) (width 1) (layer F.Cu) (net 13))
  (segment (start 80.01 71.12) (end 77.47 68.58) (width 1) (layer F.Cu) (net 13))
  (segment (start 77.47 68.58) (end 76.2 68.58) (width 1) (layer F.Cu) (net 13))
  (segment (start 67.31 71.12) (end 76.2 71.12) (width 1) (layer F.Cu) (net 14))
  (segment (start 77.47 72.39) (end 77.47 80.01) (width 1) (layer F.Cu) (net 14))
  (segment (start 76.2 71.12) (end 77.47 72.39) (width 1) (layer F.Cu) (net 14))
  (segment (start 59.69 63.5) (end 54.61 63.5) (width 1) (layer B.Cu) (net 15) (status 30))
  (segment (start 54.61 66.04) (end 59.69 66.04) (width 1) (layer B.Cu) (net 16) (status 30))
  (segment (start 59.69 68.58) (end 54.61 68.58) (width 1) (layer B.Cu) (net 17) (status 30))
  (segment (start 57.15 34.29) (end 53.34 34.29) (width 1) (layer B.Cu) (net 18) (status 10))
  (segment (start 52.07 33.02) (end 52.07 27.94) (width 1) (layer B.Cu) (net 18) (status 20))
  (segment (start 53.34 34.29) (end 52.07 33.02) (width 1) (layer B.Cu) (net 18))
  (segment (start 59.69 34.29) (end 59.69 27.94) (width 1) (layer B.Cu) (net 19) (status 30))
  (segment (start 76.2 17.78) (end 78.74 17.78) (width 1) (layer B.Cu) (net 20) (status 30))
  (segment (start 101.6 24.13) (end 101.6 22.86) (width 1) (layer B.Cu) (net 20) (status 20))
  (segment (start 76.2 17.78) (end 76.2 21.59) (width 1) (layer B.Cu) (net 20) (status 10))
  (segment (start 76.2 21.59) (end 80.01 25.4) (width 1) (layer B.Cu) (net 20))
  (segment (start 80.01 25.4) (end 100.33 25.4) (width 1) (layer B.Cu) (net 20))
  (segment (start 100.33 25.4) (end 101.6 24.13) (width 1) (layer B.Cu) (net 20))
  (segment (start 106.81863 76.2) (end 105.54863 74.93) (width 1) (layer B.Cu) (net 20))
  (segment (start 107.95 76.2) (end 106.81863 76.2) (width 1) (layer B.Cu) (net 20) (status 10))
  (segment (start 105.54863 74.93) (end 105.54863 54.47137) (width 1) (layer B.Cu) (net 20))
  (segment (start 109.22 50.8) (end 113.03 50.8) (width 1) (layer B.Cu) (net 20) (status 20))
  (segment (start 105.54863 54.47137) (end 109.22 50.8) (width 1) (layer B.Cu) (net 20))
  (segment (start 113.03 50.8) (end 113.03 53.34) (width 1) (layer B.Cu) (net 20) (status 30))
  (segment (start 104.72 22.86) (end 102.73137 22.86) (width 1) (layer B.Cu) (net 20))
  (segment (start 102.73137 22.86) (end 101.6 22.86) (width 1) (layer B.Cu) (net 20) (status 20))
  (segment (start 113.03 31.17) (end 104.72 22.86) (width 1) (layer B.Cu) (net 20))
  (segment (start 113.03 33.02) (end 113.03 31.17) (width 1) (layer B.Cu) (net 20) (status 10))
  (segment (start 110.49 33.02) (end 113.03 33.02) (width 1) (layer F.Cu) (net 20) (status 20))
  (segment (start 109.22 34.29) (end 110.49 33.02) (width 1) (layer F.Cu) (net 20))
  (segment (start 109.22 46.99) (end 109.22 34.29) (width 1) (layer F.Cu) (net 20))
  (segment (start 113.03 50.8) (end 109.22 46.99) (width 1) (layer F.Cu) (net 20) (status 10))
  (segment (start 49.53 60.96) (end 59.69 60.96) (width 1) (layer B.Cu) (net 21) (status 30))
  (segment (start 99.06 17.78) (end 99.06 22.86) (width 1) (layer B.Cu) (net 22) (tstamp 5CE42867) (status 30))
  (segment (start 96.52 22.86) (end 96.52 17.78) (width 1) (layer B.Cu) (net 23) (tstamp 5CE4286A) (status 30))
  (segment (start 93.98 17.78) (end 93.98 22.86) (width 1) (layer B.Cu) (net 24) (tstamp 5CE4286D) (status 30))
  (segment (start 91.44 22.86) (end 91.44 17.78) (width 1) (layer B.Cu) (net 25) (tstamp 5CE42870) (status 30))
  (segment (start 88.9 17.78) (end 88.9 22.86) (width 1) (layer B.Cu) (net 26) (tstamp 5CE42873) (status 30))
  (segment (start 86.36 22.86) (end 86.36 17.78) (width 1) (layer B.Cu) (net 27) (tstamp 5CE42876) (status 30))
  (segment (start 83.82 17.78) (end 83.82 22.86) (width 1) (layer B.Cu) (net 28) (tstamp 5CE42879) (status 30))
  (segment (start 81.28 22.86) (end 81.28 17.78) (width 1) (layer B.Cu) (net 29) (tstamp 5CE4287C) (status 30))
  (segment (start 87.63 66.04) (end 85.09 66.04) (width 1) (layer B.Cu) (net 30) (status 10))
  (segment (start 85.09 66.04) (end 82.55 63.5) (width 1) (layer B.Cu) (net 30))
  (segment (start 82.55 63.5) (end 71.12 63.5) (width 1) (layer B.Cu) (net 30))
  (segment (start 71.12 63.5) (end 68.58 66.04) (width 1) (layer B.Cu) (net 30))
  (segment (start 68.58 66.04) (end 67.31 66.04) (width 1) (layer B.Cu) (net 30) (status 20))
  (segment (start 83.82 43.18) (end 83.82 58.42) (width 1) (layer F.Cu) (net 31) (status 10))
  (segment (start 83.82 58.42) (end 87.63 58.42) (width 1) (layer F.Cu) (net 31) (status 20))
  (segment (start 83.82 62.23) (end 83.82 58.42) (width 1) (layer F.Cu) (net 31))
  (segment (start 82.55 63.5) (end 83.82 62.23) (width 1) (layer F.Cu) (net 31))
  (segment (start 67.31 63.5) (end 82.55 63.5) (width 1) (layer F.Cu) (net 31) (status 10))
  (segment (start 87.63 60.96) (end 67.31 60.96) (width 1) (layer B.Cu) (net 32) (status 30))
  (segment (start 88.76137 60.96) (end 87.63 60.96) (width 1) (layer F.Cu) (net 32) (status 20))
  (segment (start 89.430001 60.291369) (end 88.76137 60.96) (width 1) (layer F.Cu) (net 32))
  (segment (start 89.430001 52.475999) (end 89.430001 60.291369) (width 1) (layer F.Cu) (net 32))
  (segment (start 86.36 49.405998) (end 89.430001 52.475999) (width 1) (layer F.Cu) (net 32))
  (segment (start 86.36 43.18) (end 86.36 49.405998) (width 1) (layer F.Cu) (net 32) (status 10))
  (segment (start 49.53 35.56) (end 49.53 27.94) (width 1) (layer F.Cu) (net 33) (status 20))
  (segment (start 52.07 38.1) (end 49.53 35.56) (width 1) (layer F.Cu) (net 33))
  (segment (start 60.96 38.1) (end 52.07 38.1) (width 1) (layer F.Cu) (net 33))
  (segment (start 67.31 48.26) (end 63.5 48.26) (width 1) (layer F.Cu) (net 33) (status 10))
  (segment (start 63.5 48.26) (end 62.23 46.99) (width 1) (layer F.Cu) (net 33))
  (segment (start 62.23 46.99) (end 62.23 39.37) (width 1) (layer F.Cu) (net 33))
  (segment (start 62.23 39.37) (end 60.96 38.1) (width 1) (layer F.Cu) (net 33))
  (segment (start 67.31 45.72) (end 64.77 45.72) (width 1) (layer F.Cu) (net 34) (status 10))
  (segment (start 62.23 31.75) (end 62.23 27.94) (width 1) (layer F.Cu) (net 34) (status 20))
  (segment (start 64.77 34.29) (end 62.23 31.75) (width 1) (layer F.Cu) (net 34))
  (segment (start 64.77 45.72) (end 64.77 34.29) (width 1) (layer F.Cu) (net 34))
  (segment (start 96.52 30.48) (end 96.52 35.56) (width 1) (layer B.Cu) (net 35) (tstamp 5CE42723) (status 30))
  (segment (start 93.98 35.56) (end 93.98 30.48) (width 1) (layer B.Cu) (net 36) (tstamp 5CE42720) (status 30))
  (segment (start 91.44 30.48) (end 91.44 35.56) (width 1) (layer B.Cu) (net 37) (tstamp 5CE4271D) (status 30))
  (segment (start 88.9 35.56) (end 88.9 30.48) (width 1) (layer B.Cu) (net 38) (tstamp 5CE4271A) (status 30))
  (segment (start 86.36 30.48) (end 86.36 35.56) (width 1) (layer B.Cu) (net 39) (tstamp 5CE42717) (status 30))
  (segment (start 83.82 35.56) (end 83.82 30.48) (width 1) (layer B.Cu) (net 40) (tstamp 5CE42714) (status 30))
  (segment (start 81.28 35.56) (end 81.28 30.48) (width 1) (layer B.Cu) (net 41) (tstamp 5CE42711) (status 30))
  (segment (start 99.06 30.48) (end 99.06 38.1) (width 1) (layer B.Cu) (net 42) (tstamp 5CE4270E) (status 10))
  (segment (start 93.98 40.64) (end 93.98 43.18) (width 1) (layer B.Cu) (net 42) (tstamp 5CE4270B) (status 20))
  (segment (start 97.79 39.37) (end 95.25 39.37) (width 1) (layer B.Cu) (net 42) (tstamp 5CE42642))
  (segment (start 99.06 38.1) (end 97.79 39.37) (width 1) (layer B.Cu) (net 42) (tstamp 5CE4263F))
  (segment (start 95.25 39.37) (end 93.98 40.64) (width 1) (layer B.Cu) (net 42) (tstamp 5CE4263C))
  (segment (start 100.33 73.66) (end 92.71 73.66) (width 1) (layer B.Cu) (net 43) (tstamp 5CE426F9) (status 10))
  (segment (start 92.71 73.66) (end 91.44 72.39) (width 1) (layer B.Cu) (net 43) (tstamp 5CE426F6))
  (segment (start 91.44 72.39) (end 91.44 69.85) (width 1) (layer B.Cu) (net 43) (tstamp 5CE426F3))
  (segment (start 91.44 69.85) (end 90.17 68.58) (width 1) (layer B.Cu) (net 43) (tstamp 5CE426F0))
  (segment (start 90.17 68.58) (end 87.63 68.58) (width 1) (layer B.Cu) (net 43) (tstamp 5CE42708) (status 20))
  (segment (start 95.25 55.88) (end 100.33 55.88) (width 1) (layer B.Cu) (net 44) (tstamp 5CE42705) (status 30))
  (segment (start 100.33 58.42) (end 95.25 58.42) (width 1) (layer B.Cu) (net 45) (tstamp 5CE42702) (status 30))
  (segment (start 95.25 60.96) (end 100.33 60.96) (width 1) (layer B.Cu) (net 46) (tstamp 5CE426FF) (status 30))
  (segment (start 100.33 63.5) (end 95.25 63.5) (width 1) (layer B.Cu) (net 47) (tstamp 5CE426FC) (status 30))
  (segment (start 95.25 66.04) (end 100.33 66.04) (width 1) (layer B.Cu) (net 48) (tstamp 5CE426ED) (status 30))
  (segment (start 100.33 68.58) (end 95.25 68.58) (width 1) (layer B.Cu) (net 49) (tstamp 5CE426EA) (status 30))
  (segment (start 95.25 71.12) (end 100.33 71.12) (width 1) (layer B.Cu) (net 50) (tstamp 5CE426E7) (status 30))
  (segment (start 113.03 55.88) (end 107.95 55.88) (width 1) (layer B.Cu) (net 51) (tstamp 5CE425A3) (status 30))
  (segment (start 107.95 58.42) (end 113.03 58.42) (width 1) (layer B.Cu) (net 52) (tstamp 5CE425AF) (status 30))
  (segment (start 107.95 60.96) (end 113.03 60.96) (width 1) (layer B.Cu) (net 53) (tstamp 5CE425A9) (status 30))
  (segment (start 107.95 63.5) (end 113.03 63.5) (width 1) (layer B.Cu) (net 54) (tstamp 5CE425AC) (status 30))
  (segment (start 107.95 66.04) (end 113.03 66.04) (width 1) (layer B.Cu) (net 55) (tstamp 5CE42645) (status 30))
  (segment (start 107.95 68.58) (end 113.03 68.58) (width 1) (layer B.Cu) (net 56) (tstamp 5CE425A6) (status 30))
  (segment (start 107.95 71.12) (end 113.03 71.12) (width 1) (layer B.Cu) (net 57) (tstamp 5CE425E2) (status 30))
  (segment (start 107.95 73.66) (end 113.03 73.66) (width 1) (layer B.Cu) (net 58) (tstamp 5CE425A0) (status 30))
  (via (at 72.39 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 59))
  (via (at 104.14 50.8) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 59) (tstamp 5CE4519F))
  (via (at 105.41 19.05) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 59) (tstamp 5CE451A1))
  (segment (start 54.53 25.32) (end 54.61 25.4) (width 1) (layer B.Cu) (net 59))
  (segment (start 39.37 25.32) (end 54.53 25.32) (width 1) (layer B.Cu) (net 59) (status 10))
  (segment (start 54.61 25.4) (end 54.61 20.32) (width 1) (layer B.Cu) (net 59) (status 20))
  (segment (start 54.61 27.94) (end 54.61 25.4) (width 1) (layer B.Cu) (net 59) (status 10))
  (segment (start 54.61 25.4) (end 57.15 25.4) (width 1) (layer B.Cu) (net 59))
  (segment (start 57.15 25.4) (end 57.15 27.94) (width 1) (layer B.Cu) (net 59) (status 20))
  (segment (start 57.15 20.32) (end 57.15 25.4) (width 1) (layer B.Cu) (net 59) (status 10))
  (segment (start 57.15 25.4) (end 67.31 25.4) (width 1) (layer B.Cu) (net 59))
  (segment (start 67.31 25.4) (end 71.12 29.21) (width 1) (layer B.Cu) (net 59))
  (segment (start 101.6 30.48) (end 101.6 27.94) (width 1) (layer B.Cu) (net 59) (status 10))
  (segment (start 72.39 27.94) (end 71.12 29.21) (width 1) (layer B.Cu) (net 59))
  (segment (start 101.6 27.94) (end 72.39 27.94) (width 1) (layer B.Cu) (net 59))
  (segment (start 102.399999 31.279999) (end 101.6 30.48) (width 1) (layer F.Cu) (net 59) (status 30))
  (segment (start 103.200001 32.080001) (end 102.399999 31.279999) (width 1) (layer F.Cu) (net 59) (status 20))
  (segment (start 103.200001 73.329999) (end 103.200001 32.080001) (width 1) (layer F.Cu) (net 59))
  (segment (start 100.33 76.2) (end 103.200001 73.329999) (width 1) (layer F.Cu) (net 59) (status 10))
  (segment (start 71.755 30.653614) (end 71.755 31.33499) (width 1) (layer B.Cu) (net 59) (status 20))
  (segment (start 71.12 30.018614) (end 71.755 30.653614) (width 1) (layer B.Cu) (net 59))
  (segment (start 71.12 29.21) (end 71.12 30.018614) (width 1) (layer B.Cu) (net 59))
  (via (at 114.935 46.99) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 59) (tstamp 5CE451F6))
  (segment (start 87.63 53.34) (end 87.63 50.8) (width 1) (layer B.Cu) (net 60) (status 10))
  (segment (start 91.44 46.99) (end 91.44 43.18) (width 1) (layer B.Cu) (net 60) (status 20))
  (segment (start 87.63 50.8) (end 91.44 46.99) (width 1) (layer B.Cu) (net 60))
  (segment (start 53.34 40.64) (end 59.69 40.64) (width 1.5) (layer B.Cu) (net 61))

  (zone (net 1) (net_name GNDD) (layer B.Cu) (tstamp 5CE45A98) (hatch edge 0.508)
    (connect_pads (clearance 1))
    (min_thickness 0.5)
    (fill (arc_segments 16) (thermal_gap 1) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 12.7 12.7) (xy 34.29 12.7) (xy 34.29 25.4) (xy 41.91 30.48) (xy 46.99 30.48)
        (xy 49.53 33.02) (xy 97.79 33.02) (xy 97.79 43.18) (xy 97.79 46.99) (xy 97.79 49.53)
        (xy 97.79 82.55) (xy 12.7 82.55)
      )
    )
  )
  (zone (net 59) (net_name GNDPWR) (layer B.Cu) (tstamp 5CE45A95) (hatch edge 0.508)
    (connect_pads (clearance 1))
    (min_thickness 0.5)
    (fill (arc_segments 16) (thermal_gap 1) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 35.56 12.7) (xy 116.84 12.7) (xy 116.84 82.55) (xy 99.06 82.55) (xy 99.06 50.8)
        (xy 101.6 48.26) (xy 114.3 48.26) (xy 114.3 29.21) (xy 110.49 29.21) (xy 104.775 31.75)
        (xy 55.245 31.75) (xy 50.8 31.75) (xy 48.26 29.21) (xy 43.18 29.21) (xy 35.56 24.13)
      )
    )
  )
  (zone (net 1) (net_name GNDD) (layer F.Cu) (tstamp 5CE45A92) (hatch edge 0.508)
    (connect_pads (clearance 1))
    (min_thickness 0.3)
    (fill (arc_segments 16) (thermal_gap 1) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 12.7 12.7) (xy 34.29 12.7) (xy 34.29 25.4) (xy 41.91 30.48) (xy 46.99 30.48)
        (xy 49.53 33.02) (xy 97.79 33.02) (xy 97.79 43.18) (xy 97.79 82.55) (xy 12.7 82.55)
      )
    )
  )
  (zone (net 59) (net_name GNDPWR) (layer F.Cu) (tstamp 5CE45A8F) (hatch edge 0.508)
    (connect_pads (clearance 1))
    (min_thickness 0.3)
    (fill (arc_segments 16) (thermal_gap 1) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 35.56 12.7) (xy 116.84 12.7) (xy 116.84 82.55) (xy 99.06 82.55) (xy 99.06 50.8)
        (xy 99.06 48.26) (xy 99.06 31.75) (xy 50.8 31.75) (xy 48.26 29.21) (xy 43.18 29.21)
        (xy 35.56 24.13)
      )
    )
  )
)
