(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu16.04.1)

  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 225)
    (zones 0)
    (modules 20)
    (nets 18)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.3)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 0.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plots/"))
  )

  (net 0 "")
  (net 1 +15V)
  (net 2 GNDA)
  (net 3 -15V)
  (net 4 "Net-(RA3-Pad2)")
  (net 5 "Net-(RB3-Pad2)")
  (net 6 inB+)
  (net 7 inA+)
  (net 8 inB-)
  (net 9 inA-)
  (net 10 outA)
  (net 11 outB)
  (net 12 "Net-(JA2-Pad2)")
  (net 13 "Net-(JB1-Pad2)")
  (net 14 "Net-(ClpA1-Pad1)")
  (net 15 "Net-(ClpA1-Pad2)")
  (net 16 "Net-(ClpB1-Pad2)")
  (net 17 "Net-(ClpB1-Pad1)")

  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(ClpA1-Pad1)")
    (add_net "Net-(ClpA1-Pad2)")
    (add_net "Net-(ClpB1-Pad1)")
    (add_net "Net-(ClpB1-Pad2)")
    (add_net "Net-(JA2-Pad2)")
    (add_net "Net-(JB1-Pad2)")
    (add_net "Net-(RA3-Pad2)")
    (add_net "Net-(RB3-Pad2)")
    (add_net inA+)
    (add_net inA-)
    (add_net inB+)
    (add_net inB-)
    (add_net outA)
    (add_net outB)
  )

  (net_class power ""
    (clearance 0.3)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +15V)
    (add_net -15V)
    (add_net GNDA)
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5D4D76E4)
    (at 99.06 36.83 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5CA39C35)
    (fp_text reference RA6 (at -2.54 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0|0|220 (at 12.7 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(ClpA1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 outA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5A02E8C5) (tstamp 5CA24E4D)
    (at 101.6 39.37)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (path /5C54CA7D)
    (fp_text reference U1 (at 3.81 1.905) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LM4562 (at 3.81 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 8.89) (end 0.635 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 8.89) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 8.95) (end 6.46 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 8.95) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.55) (end -1.1 9.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 9.15) (end 8.7 9.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 9.15) (end 8.7 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(ClpA1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(RB3-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(ClpA1-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(ClpB1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(RA3-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(ClpB1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 -15V))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +15V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PCIexpress_1x_letters (layer F.Cu) (tedit 5D08B442) (tstamp 5C54794C)
    (at 96.52 66.04)
    (descr "PCIexpress Bus Edge Connector")
    (tags "PCIexpress Bus Edge Connector")
    (path /5C5482AB)
    (attr virtual)
    (fp_text reference J3 (at 11.43 -4.318) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_02x18_Row_Letter_First (at 10.16 6.35) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 19.95 4.05) (end -0.95 4.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 19.95 4.05) (end 19.95 -5.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -5.45) (end -0.95 4.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -5.45) (end 19.95 -5.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start 19.7 -2) (end 19.7 3.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.4 -2) (end 12.4 3.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.4 3.8) (end 19.7 3.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 19.7 -2) (end 12.4 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 3.8) (end -0.7 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.6 3.8) (end -0.7 3.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.6 -2) (end 10.6 3.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -2) (end 10.6 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.4 -5.2) (end 12.4 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.6 -5.2) (end 12.4 -5.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.6 -2) (end 10.6 -5.2) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 9.5 0.662) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad "" connect oval (at 1 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 19 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 18 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 13 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 10 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 17 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 14 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 2 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 16 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 15 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 9 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 8 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 7 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 6 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 5 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 4 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect oval (at 3 2.8 90) (size 0.65 0.65) (layers B.Cu B.Mask))
    (pad "" connect circle (at 1 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 17 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 16 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 15 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 14 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 13 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 0 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 10 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 9 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 8 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 7 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 6 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 5 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 4 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 3 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad "" connect circle (at 2 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
    (pad 13a connect rect (at 14 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 2 GNDA))
    (pad 12a connect rect (at 13 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 9 inA-))
    (pad 18a connect rect (at 19 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 6 inB+))
    (pad 17a connect rect (at 18 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 2 GNDA))
    (pad 16a connect rect (at 17 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 8 inB-))
    (pad 15a connect rect (at 16 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 2 GNDA))
    (pad 14a connect rect (at 15 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 7 inA+))
    (pad 11a connect rect (at 10 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 2 GNDA))
    (pad 10a connect rect (at 9 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 2 GNDA))
    (pad 9a connect rect (at 8 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 1 +15V))
    (pad 8a connect rect (at 7 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 1 +15V))
    (pad 7a connect rect (at 6 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 1 +15V))
    (pad 6a connect rect (at 5 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 2 GNDA))
    (pad 5a connect rect (at 4 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 2 GNDA))
    (pad 4a connect rect (at 3 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 2 GNDA))
    (pad 3a connect rect (at 2 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 3 -15V))
    (pad 2a connect rect (at 1 0.5) (size 0.65 4.6) (layers B.Cu B.Mask)
      (net 3 -15V))
    (pad 1a connect rect (at 0 0) (size 0.65 3.6) (layers B.Cu B.Mask)
      (net 3 -15V))
    (pad 13b connect rect (at 14 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 10 outA))
    (pad 12b connect rect (at 13 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 2 GNDA))
    (pad 18b connect rect (at 19 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 2 GNDA))
    (pad 17b connect rect (at 18 0) (size 0.65 3.6) (layers F.Cu F.Mask)
      (net 11 outB))
    (pad 16b connect rect (at 17 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 11 outB))
    (pad 15b connect rect (at 16 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 2 GNDA))
    (pad 14b connect rect (at 15 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 10 outA))
    (pad 11b connect rect (at 10 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 2 GNDA))
    (pad 10b connect rect (at 9 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 2 GNDA))
    (pad 9b connect rect (at 8 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 1 +15V))
    (pad 8b connect rect (at 7 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 1 +15V))
    (pad 7b connect rect (at 6 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 1 +15V))
    (pad 6b connect rect (at 5 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 2 GNDA))
    (pad 5b connect rect (at 4 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 2 GNDA))
    (pad 4b connect rect (at 3 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 2 GNDA))
    (pad 3b connect rect (at 2 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 3 -15V))
    (pad 2b connect rect (at 1 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 3 -15V))
    (pad 1b connect rect (at 0 0.5) (size 0.65 4.6) (layers F.Cu F.Mask)
      (net 3 -15V))
    (pad "" connect circle (at 19 2.8) (size 0.65 0.65) (layers F.Cu F.Mask))
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24D4F)
    (at 96.52 54.61 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CA8C)
    (fp_text reference RA2 (at -2.54 -2.54 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k|0|open (at -7.62 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 inA-))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(ClpA1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24B48)
    (at 91.44 44.45)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAA4)
    (fp_text reference RA3 (at 3.81 -1.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k|1k|10k (at -6.35 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(RA3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 inA+))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24BBD)
    (at 93.98 46.99 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAB9)
    (fp_text reference RA4 (at 10.16 -2.54 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10|0|open (at 15.24 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0 270) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(JA2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24D91)
    (at 99.06 46.99 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAAC)
    (fp_text reference RA5 (at 10.16 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k|open|open (at 16.51 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(RA3-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24E06)
    (at 119.38 41.91 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CB19)
    (fp_text reference RB1 (at 3.81 -1.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k|10k|0 (at -6.35 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(ClpB1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 "Net-(ClpB1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24C29)
    (at 114.3 57.15 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAD8)
    (fp_text reference RB2 (at 1.905 -1.905 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k|0|open (at -6.35 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 inB-))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(ClpB1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24AD9)
    (at 119.38 46.99 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAE4)
    (fp_text reference RB3 (at 3.81 1.905 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k|1k|10k (at -6.35 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0 180) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(RB3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 inB+))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24C6B)
    (at 116.84 49.53 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAF8)
    (fp_text reference RB4 (at 3.81 -1.92 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10|0|open (at 12.7 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0 270) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(JB1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24CF2)
    (at 111.76 52.07 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAEC)
    (fp_text reference RB5 (at 3.81 -1.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k|open|open (at 5.08 -1.905 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(RB3-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA24CAD)
    (at 91.44 39.37)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CA95)
    (fp_text reference RA1 (at 3.81 1.905) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k|10k|0 (at -6.35 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(ClpA1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(ClpA1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CA24838)
    (at 109.18 36.83 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (path /5C54CB2B)
    (fp_text reference C1 (at 1.23 3.81 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 1.25 2.05 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +15V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CA24849)
    (at 104.14 49.53 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (path /5C54CB3A)
    (fp_text reference C2 (at -2.54 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at -1.27 2.05 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.25 0 180) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 -15V))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CA2485C)
    (at 99.06 33.655 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (path /5CA42A5F)
    (fp_text reference ClpA1 (at -3.175 0.635 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330p (at 2.5 3 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 -1.75) (end -1 1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1 1.75) (end 6 1.75) (layer F.Fab) (width 0.1))
    (fp_line (start 6 1.75) (end 6 -1.75) (layer F.Fab) (width 0.1))
    (fp_line (start 6 -1.75) (end -1 -1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1.12 -1.87) (end 6.12 -1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.12 1.87) (end 6.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.12 -1.87) (end -1.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.12 -1.87) (end 6.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -2) (end -1.25 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 2) (end 6.25 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.25 2) (end 6.25 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.25 -2) (end -1.25 -2) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(ClpA1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(ClpA1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CA2486F)
    (at 111.76 36.195)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (path /5CA46ED4)
    (fp_text reference ClpB1 (at 2.5 -3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330p (at 8.89 -1.905) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 6.25 -2) (end -1.25 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.25 2) (end 6.25 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 2) (end 6.25 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -2) (end -1.25 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.12 -1.87) (end 6.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.12 -1.87) (end -1.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.12 1.87) (end 6.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.12 -1.87) (end 6.12 -1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 6 -1.75) (end -1 -1.75) (layer F.Fab) (width 0.1))
    (fp_line (start 6 1.75) (end 6 -1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1 1.75) (end 6 1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -1.75) (end -1 1.75) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(ClpB1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(ClpB1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA2489D)
    (at 111.76 39.37)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5CA3D551)
    (fp_text reference RB6 (at 7.62 -1.905) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0|0|220 (at 12.7 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 "Net-(ClpB1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 outB))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5CB36154) (tstamp 5CA25528)
    (at 92.075 41.91)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (path /5C54CACC)
    (attr virtual)
    (fp_text reference JA2 (at 3.175 0) (layer B.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Jumper (at 0 -1.9) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.65 -1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.7 1) (end 0.7 1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.4 0.3) (end 1.4 -0.3) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.7 -1) (end -0.7 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.3) (end -1.4 0.3) (layer B.SilkS) (width 0.12))
    (fp_arc (start -0.7 0.3) (end -0.7 1) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start -0.7 -0.3) (end -1.4 -0.3) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start 0.7 -0.3) (end 0.7 -1) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start 0.7 0.3) (end 1.4 0.3) (angle 90) (layer B.SilkS) (width 0.12))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 12 "Net-(JA2-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 7 inA+) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )

  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5CB3615E) (tstamp 5CA2553A)
    (at 118.745 44.45 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (path /5C54CB0B)
    (attr virtual)
    (fp_text reference JB1 (at 3.175 0 180) (layer B.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Jumper (at 0 -1.9 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_arc (start 0.7 0.3) (end 1.4 0.3) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start 0.7 -0.3) (end 0.7 -1) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start -0.7 -0.3) (end -1.4 -0.3) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start -0.7 0.3) (end -0.7 1) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.3) (end -1.4 0.3) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.7 -1) (end -0.7 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.4 0.3) (end 1.4 -0.3) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.7 1) (end 0.7 1) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.65 1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 6 inB+) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 13 "Net-(JB1-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )

  (gr_line (start 108.9152 69.85) (end 116.2304 69.85) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 108.9152 61.35) (end 108.9152 69.85) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.1372 61.35) (end 108.9152 61.35) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.1372 69.85) (end 107.1372 61.35) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.682 31.623) (end 122.682 61.35) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.773 31.623) (end 122.682 31.623) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.773 61.35) (end 88.773 31.623) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8088 61.35) (end 88.773 61.35) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8088 69.85) (end 95.8088 61.35) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.1118 69.85) (end 95.8088 69.85) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.2304 61.35) (end 116.2304 69.85) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.682 61.35) (end 116.2304 61.35) (layer Edge.Cuts) (width 0.1))
  (gr_text "A unbalanced" (at 96.774 41.91) (layer B.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.15)) (justify mirror))
  )
  (gr_text "B unbalanced" (at 114.046 44.45) (layer B.SilkS) (tstamp 5D2461CE)
    (effects (font (size 0.6 0.6) (thickness 0.15)) (justify mirror))
  )
  (gr_text "G   G   G" (at 112.522 63.5) (layer B.SilkS)
    (effects (font (size 0.62 0.62) (thickness 0.155)) (justify mirror))
  )
  (gr_text Out (at 112.395 60.96) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text In (at 112.395 60.96) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_text "B+ B- A- A+" (at 112.395 62.865) (layer B.SilkS)
    (effects (font (size 0.65 0.65) (thickness 0.125)) (justify mirror))
  )
  (gr_text "A     B" (at 112.522 62.738) (layer F.SilkS)
    (effects (font (size 0.65 0.65) (thickness 0.1625)))
  )
  (gr_text "- G + G" (at 101.6 62.23) (layer F.SilkS) (tstamp 5CB3648E)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "G + G -" (at 101.6 62.23) (layer B.SilkS) (tstamp 5CB36574)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_text "[ ]Input\n[ ]Output" (at 100.965 57.15) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify left))
  )

  (segment (start 103.52 62.245) (end 103.505 62.23) (width 0.5) (layer B.Cu) (net 1))
  (via (at 103.505 62.23) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 1))
  (segment (start 109.22 36.87) (end 109.18 36.83) (width 0.5) (layer F.Cu) (net 1) (status 30))
  (segment (start 109.22 39.37) (end 109.22 36.87) (width 1) (layer F.Cu) (net 1) (status 30))
  (segment (start 103.505 54.703002) (end 106.045 52.163002) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 103.505 62.23) (end 103.505 54.703002) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 106.045 52.163002) (end 106.045 40.64) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 107.315 39.37) (end 106.045 40.64) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 109.22 39.37) (end 107.315 39.37) (width 0.5) (layer F.Cu) (net 1) (status 10))
  (segment (start 103.505 66.525) (end 103.52 66.54) (width 0.5) (layer B.Cu) (net 1) (status 30))
  (segment (start 103.505 62.23) (end 103.505 66.525) (width 0.5) (layer B.Cu) (net 1) (status 20))
  (segment (start 102.52 63.215) (end 103.505 62.23) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 102.52 66.54) (end 102.52 63.215) (width 0.5) (layer B.Cu) (net 1) (status 10))
  (segment (start 104.52 63.245) (end 103.505 62.23) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 104.52 66.54) (end 104.52 63.245) (width 0.5) (layer B.Cu) (net 1) (status 10))
  (segment (start 102.52 63.215) (end 103.505 62.23) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 102.52 66.54) (end 102.52 63.215) (width 0.5) (layer F.Cu) (net 1) (status 10))
  (segment (start 103.52 62.245) (end 103.505 62.23) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 103.52 66.54) (end 103.52 62.245) (width 0.5) (layer F.Cu) (net 1) (status 10))
  (segment (start 104.52 63.245) (end 103.505 62.23) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 104.52 66.54) (end 104.52 63.245) (width 0.5) (layer F.Cu) (net 1) (status 10))
  (segment (start 104.1 49.53) (end 104.1 53.38) (width 1) (layer B.Cu) (net 2) (tstamp 5CA24D22) (status 10))
  (segment (start 104.1 53.38) (end 102.87 54.61) (width 1) (layer B.Cu) (net 2) (tstamp 5CA24D1F))
  (segment (start 100.33 54.61) (end 99.06 54.61) (width 1) (layer B.Cu) (net 2) (tstamp 5CA24CDA) (status 20))
  (segment (start 93.98 54.61) (end 93.98 53.34) (width 0.5) (layer B.Cu) (net 2) (tstamp 5CA24C11) (status 10))
  (segment (start 95.25 52.07) (end 97.79 52.07) (width 0.5) (layer B.Cu) (net 2) (tstamp 5CA24C0E))
  (segment (start 93.98 53.34) (end 95.25 52.07) (width 0.5) (layer B.Cu) (net 2) (tstamp 5CA24C0B))
  (segment (start 99.06 53.34) (end 99.06 54.61) (width 0.5) (layer B.Cu) (net 2) (tstamp 5CA24C08) (status 20))
  (segment (start 97.79 52.07) (end 99.06 53.34) (width 0.5) (layer B.Cu) (net 2) (tstamp 5CA24C05))
  (segment (start 116.84 57.15) (end 116.84 55.88) (width 0.5) (layer B.Cu) (net 2) (tstamp 5CA24C02) (status 10))
  (segment (start 116.84 55.88) (end 115.57 54.61) (width 0.5) (layer B.Cu) (net 2) (tstamp 5CA24BFF))
  (segment (start 102.87 54.61) (end 101.6 54.61) (width 1) (layer B.Cu) (net 2))
  (via (at 105.41 54.61) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (via (at 110.49 54.61) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 100.52 63.74) (end 100.5205 63.7395) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 100.52 66.54) (end 100.52 63.74) (width 0.5) (layer B.Cu) (net 2) (status 10))
  (segment (start 100.5205 63.7395) (end 100.5205 62.2935) (width 0.5) (layer B.Cu) (net 2))
  (via (at 100.838 54.61) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 100.33 54.61) (end 100.838 54.61) (width 1) (layer B.Cu) (net 2))
  (segment (start 101.6 54.61) (end 100.838 54.61) (width 1) (layer B.Cu) (net 2))
  (segment (start 100.5205 54.9275) (end 100.838 54.61) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 99.52 66.54) (end 99.52 63.294) (width 0.5) (layer F.Cu) (net 2) (status 10))
  (segment (start 100.52 62.294) (end 100.5205 62.2935) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 100.52 66.54) (end 100.52 62.294) (width 0.5) (layer F.Cu) (net 2) (status 10))
  (segment (start 101.52 66.54) (end 101.52 63.293) (width 0.5) (layer F.Cu) (net 2) (status 10))
  (via (at 100.5205 60.96) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 100.5205 62.2935) (end 100.5205 60.96) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 100.5205 60.96) (end 100.5205 54.9275) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 100.5205 60.96) (end 93.98 60.96) (width 0.5) (layer B.Cu) (net 2))
  (via (at 91.44 58.928) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (via (at 97.79 52.07) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 104.14 39.37) (end 104.14 49.53) (width 1) (layer F.Cu) (net 2))
  (segment (start 106.68 36.83) (end 104.14 39.37) (width 1) (layer F.Cu) (net 2))
  (segment (start 104.18 53.38) (end 104.1 53.38) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 105.41 54.61) (end 104.18 53.38) (width 1) (layer B.Cu) (net 2))
  (via (at 110.52 57.404) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 105.41 54.61) (end 110.49 54.61) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 110.52 54.64) (end 110.49 54.61) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 112.52 54.735) (end 112.395 54.61) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 112.52 66.54) (end 112.52 54.735) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 112.395 54.61) (end 110.49 54.61) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 115.57 54.61) (end 112.395 54.61) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 105.52 66.54) (end 105.52 62.882) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 115.52 63.55) (end 115.52 66.54) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 106.68 36.83) (end 106.68 34.29) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 106.68 34.29) (end 107.95 33.02) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 107.95 33.02) (end 120.65 33.02) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 120.65 33.02) (end 121.530011 33.900011) (width 0.5) (layer F.Cu) (net 2))
  (via (at 121.530011 36.83) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 121.530011 33.900011) (end 121.530011 36.83) (width 0.5) (layer F.Cu) (net 2))
  (via (at 120.65 33.02) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (via (at 107.95 33.02) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (via (at 104.14 39.37) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (via (at 90.17 49.53) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 90.17 49.53) (end 93.98 49.53) (width 0.5) (layer F.Cu) (net 2))
  (via (at 93.98 49.53) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 90.17 50.095685) (end 90.17 49.53) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 93.414315 60.96) (end 90.17 57.715685) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 90.17 57.715685) (end 90.17 50.095685) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 93.98 60.96) (end 93.414315 60.96) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 93.98 50.8) (end 95.25 52.07) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 93.98 49.53) (end 93.98 50.8) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 105.52 66.54) (end 105.52 62.882) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 114.52 59.47) (end 116.84 57.15) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 114.52 66.54) (end 114.52 59.47) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 121.530011 37.395685) (end 121.530011 36.83) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 121.530011 55.496373) (end 121.530011 37.395685) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 115.52 66.54) (end 115.52 61.506384) (width 0.5) (layer F.Cu) (net 2))
  (via (at 120.12106 57.117444) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 120.015 57.011384) (end 120.12106 57.117444) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 115.52 61.506384) (end 120.015 57.011384) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 120.015 57.011384) (end 121.530011 55.496373) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 116.84 56.160051) (end 119.660051 53.34) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 116.84 57.15) (end 116.84 56.160051) (width 0.5) (layer F.Cu) (net 2))
  (via (at 119.660051 53.34) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 120.12106 53.801009) (end 119.660051 53.34) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 120.12106 57.117444) (end 120.12106 53.801009) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 99.52 63.294) (end 99.52 61.008) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 99.568 60.96) (end 100.5205 60.96) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 99.52 61.008) (end 99.568 60.96) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 101.52 63.293) (end 101.52 61.388) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 101.092 60.96) (end 100.5205 60.96) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 101.52 61.388) (end 101.092 60.96) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 105.52 62.882) (end 105.52 61.012315) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 105.52 62.882) (end 105.52 61.104) (width 0.5) (layer B.Cu) (net 2))
  (via (at 105.52 61.104) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 106.316 61.104) (end 105.52 61.104) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 106.52 61.308) (end 106.316 61.104) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 106.52 66.54) (end 106.52 61.308) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 100.5205 62.2935) (end 100.5205 60.96) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 101.092 60.96) (end 100.5205 60.96) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 101.52 61.388) (end 101.092 60.96) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 101.52 66.54) (end 101.52 61.388) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 99.52 61.008) (end 99.568 60.96) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 99.52 66.54) (end 99.52 61.008) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 111.76 57.404) (end 110.52 57.404) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 112.52 58.164) (end 111.76 57.404) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 112.52 66.54) (end 112.52 58.164) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 110.49 57.374) (end 110.52 57.404) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 110.49 54.61) (end 110.49 57.374) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 110.52 66.54) (end 110.52 57.404) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 106.52 61.308) (end 106.316 61.104) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 106.316 61.104) (end 105.52 61.104) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 106.52 66.54) (end 106.52 61.308) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 105.52 54.72) (end 105.41 54.61) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 108.595342 59.69) (end 105.52 59.69) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 109.51521 60.609868) (end 108.595342 59.69) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 109.52 65.578) (end 109.51521 65.57321) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 109.52 66.54) (end 109.52 65.578) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 105.52 61.104) (end 105.52 59.69) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 109.51521 65.57321) (end 109.51521 60.609868) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 105.52 59.69) (end 105.52 54.72) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 101.6 46.99) (end 101.6 49.53) (width 1) (layer B.Cu) (net 3) (tstamp 5CA24E84) (status 30))
  (via (at 97.52 62.23) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 3))
  (segment (start 97.52 62.23) (end 97.52 66.54) (width 0.5) (layer B.Cu) (net 3) (status 20))
  (segment (start 96.52 63.23) (end 97.52 62.23) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 96.52 66.04) (end 96.52 63.23) (width 0.5) (layer B.Cu) (net 3) (status 10))
  (segment (start 98.52 63.23) (end 97.52 62.23) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 98.52 66.54) (end 98.52 63.23) (width 0.5) (layer B.Cu) (net 3) (status 10))
  (segment (start 96.52 63.23) (end 97.52 62.23) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 96.52 66.54) (end 96.52 63.23) (width 0.5) (layer F.Cu) (net 3) (status 10))
  (segment (start 98.52 63.23) (end 97.52 62.23) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 98.52 66.54) (end 98.52 63.23) (width 0.5) (layer F.Cu) (net 3) (status 10))
  (segment (start 97.52 66.54) (end 97.52 62.23) (width 0.5) (layer F.Cu) (net 3) (status 10))
  (segment (start 97.52 60.69) (end 97.52 62.23) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 101.64 49.53) (end 95.885 49.53) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 92.075 53.34) (end 92.075 55.245) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 92.075 55.245) (end 97.52 60.69) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 95.885 49.53) (end 92.075 53.34) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 101.6 44.45) (end 99.06 44.45) (width 1) (layer B.Cu) (net 4) (tstamp 5CA24B18) (status 30))
  (segment (start 99.06 44.45) (end 99.06 46.99) (width 1) (layer B.Cu) (net 4) (tstamp 5CA24B15) (status 30))
  (segment (start 111.76 46.99) (end 109.22 46.99) (width 1) (layer B.Cu) (net 5) (tstamp 5CA24B21) (status 30))
  (segment (start 111.76 46.99) (end 111.76 52.07) (width 1) (layer B.Cu) (net 5) (tstamp 5CA24B1E) (status 30))
  (segment (start 119.41 46.96) (end 119.38 46.99) (width 1) (layer F.Cu) (net 6) (tstamp 5CA24D2B) (status 30))
  (segment (start 119.41 46.96) (end 119.38 46.99) (width 1) (layer B.Cu) (net 6) (tstamp 5CA24D28) (status 30))
  (segment (start 119.41 44.45) (end 119.41 46.96) (width 1) (layer B.Cu) (net 6) (tstamp 5CA24D25) (status 30))
  (segment (start 118.680001 47.689999) (end 119.38 46.99) (width 0.5) (layer B.Cu) (net 6))
  (segment (start 118.680001 57.160001) (end 118.680001 47.689999) (width 0.5) (layer B.Cu) (net 6))
  (segment (start 115.52 60.320002) (end 118.680001 57.160001) (width 0.5) (layer B.Cu) (net 6))
  (segment (start 115.52 66.54) (end 115.52 60.320002) (width 0.5) (layer B.Cu) (net 6))
  (segment (start 91.41 44.42) (end 91.44 44.45) (width 1) (layer B.Cu) (net 7) (tstamp 5CA24BFC) (status 30))
  (segment (start 91.41 41.91) (end 91.41 44.42) (width 1) (layer B.Cu) (net 7) (tstamp 5CA24BF9) (status 30))
  (segment (start 92.24001 46.239959) (end 91.44 45.439949) (width 0.5) (layer B.Cu) (net 7))
  (segment (start 92.24001 54.720012) (end 92.24001 46.239959) (width 0.5) (layer B.Cu) (net 7))
  (segment (start 111.52 66.54) (end 111.52 56.997998) (width 0.5) (layer B.Cu) (net 7))
  (segment (start 93.973997 56.453999) (end 92.24001 54.720012) (width 0.5) (layer B.Cu) (net 7))
  (segment (start 111.52 56.997998) (end 110.976001 56.453999) (width 0.5) (layer B.Cu) (net 7))
  (segment (start 91.44 45.439949) (end 91.44 44.45) (width 0.5) (layer B.Cu) (net 7))
  (segment (start 110.976001 56.453999) (end 93.973997 56.453999) (width 0.5) (layer B.Cu) (net 7))
  (segment (start 113.52 57.93) (end 113.52 66.54) (width 0.5) (layer B.Cu) (net 8))
  (segment (start 114.3 57.15) (end 113.52 57.93) (width 0.5) (layer B.Cu) (net 8))
  (via (at 96.52 57.724) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 9))
  (segment (start 96.52 57.87399) (end 96.52 57.724) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 109.52 63.74) (end 109.52 66.54) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 109.52 58.583998) (end 109.52 63.74) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 108.660002 57.724) (end 109.52 58.583998) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 96.52 57.724) (end 108.660002 57.724) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 96.52 54.61) (end 96.52 57.724) (width 0.5) (layer F.Cu) (net 9))
  (segment (start 110.52 60.99) (end 110.52 66.54) (width 0.5) (layer F.Cu) (net 10))
  (segment (start 111.52 66.54) (end 111.52 61.99) (width 0.5) (layer F.Cu) (net 10))
  (segment (start 90.450051 36.83) (end 90.17 37.110051) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 90.17 37.110051) (end 90.17 45.72) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 91.44 36.83) (end 90.450051 36.83) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 90.17 45.72) (end 91.44 46.99) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 111.52 61.99) (end 110.52 60.99) (width 0.5) (layer F.Cu) (net 10))
  (via (at 108.204 58.674) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 10))
  (segment (start 91.44 55.051386) (end 91.44 46.99) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 95.062614 58.674) (end 91.44 55.051386) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 108.204 58.674) (end 95.062614 58.674) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 108.204 58.674) (end 110.236 58.674) (width 0.5) (layer F.Cu) (net 10))
  (segment (start 110.52 58.958) (end 110.52 60.99) (width 0.5) (layer F.Cu) (net 10))
  (segment (start 110.236 58.674) (end 110.52 58.958) (width 0.5) (layer F.Cu) (net 10))
  (segment (start 113.52 66.54) (end 113.52 63.74) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 120.630001 40.620001) (end 120.630001 55.264999) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 119.38 39.37) (end 120.630001 40.620001) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 113.52 62.375) (end 113.52 63.74) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 114.52 66.04) (end 114.52 61.375) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 114.935 60.96) (end 113.52 62.375) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 114.52 61.375) (end 114.935 60.96) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 120.630001 55.264999) (end 114.935 60.96) (width 0.5) (layer F.Cu) (net 11))
  (segment (start 92.71 41.91) (end 93.98 43.18) (width 1) (layer B.Cu) (net 12) (tstamp 5CA24D31) (status 10))
  (segment (start 93.98 46.99) (end 93.98 43.18) (width 1) (layer B.Cu) (net 12) (tstamp 5CA24D2E) (status 10))
  (segment (start 118.11 44.45) (end 116.84 45.72) (width 1) (layer B.Cu) (net 13) (tstamp 5CA24B27) (status 10))
  (segment (start 116.84 45.72) (end 116.84 49.53) (width 1) (layer B.Cu) (net 13) (tstamp 5CA24D34) (status 20))
  (segment (start 99.06 33.655) (end 99.06 36.83) (width 1) (layer B.Cu) (net 14))
  (segment (start 99.06 36.83) (end 99.06 39.37) (width 1) (layer B.Cu) (net 14))
  (segment (start 99.06 39.37) (end 101.6 39.37) (width 1) (layer B.Cu) (net 14))
  (segment (start 94.06 38.02) (end 94.06 33.655) (width 1) (layer B.Cu) (net 15))
  (segment (start 92.71 39.37) (end 94.06 38.02) (width 1) (layer B.Cu) (net 15))
  (segment (start 91.44 39.37) (end 92.71 39.37) (width 1) (layer B.Cu) (net 15))
  (segment (start 97.95 41.91) (end 101.6 41.91) (width 1) (layer B.Cu) (net 15))
  (segment (start 94.06 38.02) (end 97.95 41.91) (width 1) (layer B.Cu) (net 15))
  (segment (start 96.52 43.34) (end 97.95 41.91) (width 1) (layer B.Cu) (net 15))
  (segment (start 96.52 46.99) (end 96.52 43.34) (width 1) (layer B.Cu) (net 15))
  (segment (start 116.76 40.56) (end 116.76 36.195) (width 1) (layer B.Cu) (net 16))
  (segment (start 119.38 41.91) (end 118.11 41.91) (width 1) (layer B.Cu) (net 16))
  (segment (start 118.11 41.91) (end 116.76 40.56) (width 1) (layer B.Cu) (net 16))
  (segment (start 109.22 44.45) (end 112.87 44.45) (width 1) (layer B.Cu) (net 16))
  (segment (start 113.03 44.29) (end 116.76 40.56) (width 1) (layer B.Cu) (net 16))
  (segment (start 112.87 44.45) (end 113.03 44.29) (width 1) (layer B.Cu) (net 16))
  (segment (start 114.3 45.88) (end 112.87 44.45) (width 1) (layer B.Cu) (net 16))
  (segment (start 114.3 49.53) (end 114.3 45.88) (width 1) (layer B.Cu) (net 16))
  (segment (start 111.76 36.195) (end 111.76 39.37) (width 1) (layer B.Cu) (net 17))
  (segment (start 111.76 39.37) (end 111.76 41.91) (width 1) (layer B.Cu) (net 17))
  (segment (start 111.76 41.91) (end 109.22 41.91) (width 1) (layer B.Cu) (net 17))

  (zone (net 2) (net_name GNDA) (layer B.Cu) (tstamp 5D09F0A8) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.9 31.75) (xy 122.555 31.75) (xy 122.4915 61.214) (xy 88.8365 61.214)
      )
    )
  )
  (zone (net 2) (net_name GNDA) (layer F.Cu) (tstamp 5D09F0A5) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.9 31.75) (xy 122.555 31.75) (xy 122.4915 61.214) (xy 88.8365 61.214)
      )
    )
  )
  (zone (net 3) (net_name -15V) (layer F.Cu) (tstamp 5D09F0A2) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.52 63.246) (xy 97.536 62.23) (xy 98.552 63.246) (xy 98.552 64.008) (xy 96.52 64.008)
      )
    )
  )
  (zone (net 1) (net_name +15V) (layer F.Cu) (tstamp 5D09F09F) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.362 63.246) (xy 103.378 61.976) (xy 104.648 63.246) (xy 104.648 64.008) (xy 102.362 64.008)
      )
    )
  )
  (zone (net 1) (net_name +15V) (layer B.Cu) (tstamp 5D09F09C) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.362 63.246) (xy 103.378 61.976) (xy 104.648 63.246) (xy 104.648 64.008) (xy 102.362 64.008)
      )
    )
  )
  (zone (net 3) (net_name -15V) (layer B.Cu) (tstamp 5D09F099) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.52 63.246) (xy 97.536 62.23) (xy 98.552 63.246) (xy 98.552 64.008) (xy 96.52 64.008)
      )
    )
  )
)
