(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu16.04.1)

  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 712)
    (zones 0)
    (modules 19)
    (nets 28)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 1)
    (trace_clearance 1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1)
    (via_drill 0.8)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 /relaysheet/Relais1)
  (net 2 +9V)
  (net 3 /relaysheet/Relais5)
  (net 4 /relaysheet/Relais2)
  (net 5 /relaysheet/Relais6)
  (net 6 /relaysheet/Relais3)
  (net 7 /relaysheet/Relais7)
  (net 8 /relaysheet/Relais4)
  (net 9 /relaysheet/Relais8)
  (net 10 GNDA)
  (net 11 /relaysheet/R1B_out)
  (net 12 /relaysheet/R1A_out)
  (net 13 /relaysheet/R1A_NC)
  (net 14 /relaysheet/R5B_out)
  (net 15 /relaysheet/R5A_out)
  (net 16 /relaysheet/R2B_out)
  (net 17 /relaysheet/R2A_out)
  (net 18 /relaysheet/R6A_out)
  (net 19 /relaysheet/R6B_out)
  (net 20 /relaysheet/R3A_out)
  (net 21 /relaysheet/R3B_out)
  (net 22 /relaysheet/R7B_out)
  (net 23 /relaysheet/R7A_out)
  (net 24 /relaysheet/R4A_out)
  (net 25 /relaysheet/R4B_out)
  (net 26 /relaysheet/R8A_out)
  (net 27 /relaysheet/R8B_out)

  (net_class Default "This is the default net class."
    (clearance 1)
    (trace_width 1)
    (via_dia 1)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +9V)
    (add_net /relaysheet/R1A_NC)
    (add_net /relaysheet/R1A_out)
    (add_net /relaysheet/R1B_out)
    (add_net /relaysheet/R2A_out)
    (add_net /relaysheet/R2B_out)
    (add_net /relaysheet/R3A_out)
    (add_net /relaysheet/R3B_out)
    (add_net /relaysheet/R4A_out)
    (add_net /relaysheet/R4B_out)
    (add_net /relaysheet/R5A_out)
    (add_net /relaysheet/R5B_out)
    (add_net /relaysheet/R6A_out)
    (add_net /relaysheet/R6B_out)
    (add_net /relaysheet/R7A_out)
    (add_net /relaysheet/R7B_out)
    (add_net /relaysheet/R8A_out)
    (add_net /relaysheet/R8B_out)
    (add_net /relaysheet/Relais1)
    (add_net /relaysheet/Relais2)
    (add_net /relaysheet/Relais3)
    (add_net /relaysheet/Relais4)
    (add_net /relaysheet/Relais5)
    (add_net /relaysheet/Relais6)
    (add_net /relaysheet/Relais7)
    (add_net /relaysheet/Relais8)
    (add_net GNDA)
  )

  (module footprints:Schroff_69001-908_Female (layer F.Cu) (tedit 5CE51DC1) (tstamp 5CD47F47)
    (at 93.86 76.21)
    (path /5CD4C71E)
    (fp_text reference J4 (at -2.55 -7.65) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Schroff 69001-908 Female" (at -2.55 -10.2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -47.5 2.5) (end -47.5 -7.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 47.5 2.5) (end -47.5 2.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 47.5 -7.5) (end 47.5 2.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -47.5 -7.5) (end 47.5 -7.5) (layer F.SilkS) (width 0.15))
    (pad "" np_thru_hole circle (at -44.63 -2.55) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 44.57 -2.55) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad 32 thru_hole circle (at 39.47 -5.1) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 31 thru_hole circle (at 39.47 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /relaysheet/R1B_out))
    (pad 30 thru_hole circle (at 34.37 -5.1) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 29 thru_hole circle (at 34.37 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /relaysheet/R1A_out))
    (pad 28 thru_hole circle (at 29.27 -5.1) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 27 thru_hole circle (at 29.27 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /relaysheet/R2B_out))
    (pad 26 thru_hole circle (at 24.17 -5.1) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 25 thru_hole circle (at 24.17 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /relaysheet/R2A_out))
    (pad 24 thru_hole circle (at 19.07 -5.1) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 23 thru_hole circle (at 19.07 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /relaysheet/R3B_out))
    (pad 22 thru_hole circle (at 13.97 -5.1) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 21 thru_hole circle (at 13.97 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /relaysheet/R3A_out))
    (pad 20 thru_hole circle (at 8.87 -5.1) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 19 thru_hole circle (at 8.87 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /relaysheet/R4B_out))
    (pad 18 thru_hole circle (at 3.77 -5.1) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 17 thru_hole circle (at 3.77 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /relaysheet/R4A_out))
    (pad 16 thru_hole circle (at -1.33 -5.1) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 15 thru_hole circle (at -1.33 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /relaysheet/R5B_out))
    (pad 14 thru_hole circle (at -6.43 -5.1) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 13 thru_hole circle (at -6.43 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /relaysheet/R5A_out))
    (pad 12 thru_hole circle (at -11.53 -5.1) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 11 thru_hole circle (at -11.53 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /relaysheet/R6B_out))
    (pad 10 thru_hole circle (at -16.63 -5.1) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 9 thru_hole circle (at -16.63 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /relaysheet/R6A_out))
    (pad 8 thru_hole circle (at -21.73 -5.1) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 7 thru_hole circle (at -21.73 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /relaysheet/R7B_out))
    (pad 6 thru_hole circle (at -26.83 -5.1) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 5 thru_hole circle (at -26.83 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /relaysheet/R7A_out))
    (pad 4 thru_hole circle (at -31.93 -5.1) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 3 thru_hole circle (at -31.93 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /relaysheet/R8B_out))
    (pad 2 thru_hole circle (at -37.03 -5.1) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 1 thru_hole rect (at -37.03 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /relaysheet/R8A_out))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2D6D0)
    (at 159.72 49.53 90)
    (path /5CD2BD35/5CD2D6AA)
    (fp_text reference U1 (at 8.89 0.3 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 12 /relaysheet/R1A_out))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 11 /relaysheet/R1B_out))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 1 /relaysheet/Relais1))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2F79B)
    (at 141.27 49.53 90)
    (path /5CD2BD35/5CD30362)
    (fp_text reference U2 (at 8.89 -0.3 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 17 /relaysheet/R2A_out))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 16 /relaysheet/R2B_out))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 4 /relaysheet/Relais2))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2D700)
    (at 123.19 49.53 90)
    (path /5CD2BD35/5CD316D2)
    (fp_text reference U3 (at 8.89 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 20 /relaysheet/R3A_out))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 21 /relaysheet/R3B_out))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 6 /relaysheet/Relais3))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD30B02)
    (at 105.31 49.53 90)
    (path /5CD2BD35/5CD31724)
    (fp_text reference U4 (at 8.89 0.1 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 8 /relaysheet/Relais4))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 25 /relaysheet/R4B_out))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 24 /relaysheet/R4A_out))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2D730)
    (at 87.33 49.53 90)
    (path /5CD2BD35/5CD2FCCA)
    (fp_text reference U5 (at 8.89 0.3 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 3 /relaysheet/Relais5))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 14 /relaysheet/R5B_out))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 15 /relaysheet/R5A_out))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2D748)
    (at 69.85 49.53 90)
    (path /5CD2BD35/5CD3038B)
    (fp_text reference U6 (at 8.89 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 5 /relaysheet/Relais6))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 19 /relaysheet/R6B_out))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 18 /relaysheet/R6A_out))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD2DE4A)
    (at 49.53 49.53 90)
    (path /5CD2BD35/5CD316FB)
    (fp_text reference U7 (at 8.89 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 7 /relaysheet/Relais7))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 22 /relaysheet/R7B_out))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 23 /relaysheet/R7A_out))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
  )

  (module footprints:NEC-EB2-12NU (layer F.Cu) (tedit 5CD1A950) (tstamp 5CD30EC6)
    (at 31.45 49.53 90)
    (path /5CD2BD35/5CD3174D)
    (fp_text reference U8 (at 8.89 0.3 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NEC-EB2-12NU (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4 -2.54) (end -4 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 2.54) (end -5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 2.54) (end -5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -2.54) (end 5.08 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -2.54) (end 5.08 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4.65) (end -6 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 4.65) (end -7.15 -4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 4.65) (end -7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start 7.15 -4.65) (end 7.15 4.65) (layer F.Fab) (width 0.15))
    (fp_line (start -7.15 -4.65) (end 7.15 -4.65) (layer F.Fab) (width 0.15))
    (pad 10 smd rect (at -5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 9 /relaysheet/Relais8))
    (pad 9 smd rect (at -2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 smd rect (at 0 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 27 /relaysheet/R8B_out))
    (pad 7 smd rect (at 2.54 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 smd rect (at 5.08 4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 smd rect (at 0 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 26 /relaysheet/R8A_out))
    (pad 2 smd rect (at -2.54 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 1 smd rect (at -5.08 -4.78 90) (size 1 2.94) (layers F.Cu F.Paste F.Mask)
      (net 2 +9V))
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F417)
    (at 154.94 58.42)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD2E7CE)
    (fp_text reference D1 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 /relaysheet/Relais1))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F435)
    (at 137.16 58.42)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD3037D)
    (fp_text reference D2 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 /relaysheet/Relais2))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F453)
    (at 119.38 58.42)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD316ED)
    (fp_text reference D3 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 /relaysheet/Relais3))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD30AAF)
    (at 101.6 58.42)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD3173F)
    (fp_text reference D4 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 /relaysheet/Relais4))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F48F)
    (at 83.82 58.42)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD2FCE5)
    (fp_text reference D5 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 /relaysheet/Relais5))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F4AD)
    (at 66.04 58.42)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD303A6)
    (fp_text reference D6 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 /relaysheet/Relais6))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD2F4CB)
    (at 45.72 58.42)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD31716)
    (fp_text reference D7 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 /relaysheet/Relais7))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CD30E70)
    (at 27.94 58.42)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5CD2BD35/5CD31768)
    (fp_text reference D8 (at 3.81 -2.47) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D (at 3.81 2.47) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 2.09 -1.35) (end 2.09 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -1.35) (end 1.89 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.09 -1.14) (end 1.09 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 -1.47) (end 6.53 -1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 -1.47) (end 6.53 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.14) (end 1.09 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.09 1.47) (end 6.53 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.53 1.47) (end 6.53 1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.47) (end 1.99 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.11 -1.47) (end 2.11 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.87 -1.47) (end 1.87 1.47) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 1.6) (end 8.77 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 1.6) (end 8.77 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.77 -1.6) (end -1.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 4.2 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user K (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +9V))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 /relaysheet/Relais8))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CE6B213)
    (at 59.69 17.78)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (path /5CE859BA)
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x10 (at 0 25.19) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 24.13) (end -1.27 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 24.13) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 24.19) (end 1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 24.65) (end 1.8 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 24.65) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 11.43 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /relaysheet/R1A_NC))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GNDA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CE3F03A)
    (at 149.86 73.66 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (path /5CE9FC06)
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x10 (at 0 25.19 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 24.13) (end -1.27 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 24.13) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 24.19) (end 1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 24.65) (end 1.8 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 24.65) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 11.43 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /relaysheet/Relais8))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /relaysheet/Relais7))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /relaysheet/Relais6))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /relaysheet/Relais5))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /relaysheet/Relais4))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /relaysheet/Relais3))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /relaysheet/Relais2))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /relaysheet/Relais1))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +9V))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +9V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text "Output Selection" (at 179.705 43.815 90) (layer F.SilkS)
    (effects (font (size 2 2) (thickness 0.3)))
  )
  (gr_text "Relais Input" (at 160.02 76.835) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Audio Input" (at 14.605 29.845 90) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 12.7 78.74) (end 12.7 12.7) (layer F.SilkS) (width 0.2))
  (gr_line (start 182.88 78.74) (end 12.7 78.74) (layer F.SilkS) (width 0.2))
  (gr_line (start 182.88 12.7) (end 182.88 78.74) (layer F.SilkS) (width 0.2))
  (gr_line (start 12.7 12.7) (end 182.88 12.7) (layer F.SilkS) (width 0.2) (tstamp 5CD2E5DF))

  (via (at 20 73) (size 5) (drill 3.1) (layers F.Cu B.Cu) (net 0))
  (via (at 178 73) (size 5) (drill 3.1) (layers F.Cu B.Cu) (net 0) (tstamp 5CE42310))
  (via (at 178 16) (size 5) (drill 3.1) (layers F.Cu B.Cu) (net 0) (tstamp 5CE42329))
  (via (at 20 16) (size 5) (drill 3.1) (layers F.Cu B.Cu) (net 0) (tstamp 5CE4234A))
  (segment (start 162.56 55.28) (end 163.23 54.61) (width 1) (layer F.Cu) (net 1) (status 20))
  (segment (start 162.56 58.42) (end 162.56 55.28) (width 1) (layer F.Cu) (net 1) (status 10))
  (segment (start 167.64 73.66) (end 167.64 71.12) (width 0.5) (layer B.Cu) (net 1) (status 10))
  (segment (start 167.64 71.12) (end 162.56 66.04) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 162.56 66.04) (end 162.56 58.42) (width 0.5) (layer B.Cu) (net 1) (status 20))
  (segment (start 27.94 55.88) (end 26.67 54.61) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 27.94 58.42) (end 27.94 55.88) (width 1) (layer F.Cu) (net 2) (status 10))
  (segment (start 45.72 55.58) (end 44.75 54.61) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 45.72 58.42) (end 45.72 55.58) (width 1) (layer F.Cu) (net 2) (status 10))
  (segment (start 66.04 55.58) (end 65.07 54.61) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 66.04 58.42) (end 66.04 55.58) (width 1) (layer F.Cu) (net 2) (status 10))
  (segment (start 83.82 55.88) (end 82.55 54.61) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 83.82 58.42) (end 83.82 55.88) (width 1) (layer F.Cu) (net 2) (status 10))
  (segment (start 101.6 55.68) (end 100.53 54.61) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 101.6 58.42) (end 101.6 55.68) (width 1) (layer F.Cu) (net 2) (status 10))
  (segment (start 119.38 55.58) (end 118.41 54.61) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 119.38 58.42) (end 119.38 55.58) (width 1) (layer F.Cu) (net 2) (status 10))
  (segment (start 154.94 55.88) (end 153.67 54.61) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 154.94 58.42) (end 154.94 55.88) (width 1) (layer F.Cu) (net 2) (status 10))
  (segment (start 170.18 73.66) (end 170.18 55.88) (width 1) (layer B.Cu) (net 2) (status 10))
  (segment (start 27.94 55.88) (end 27.94 58.42) (width 1) (layer B.Cu) (net 2) (status 20))
  (segment (start 29.21 54.61) (end 27.94 55.88) (width 1) (layer B.Cu) (net 2))
  (segment (start 45.72 58.42) (end 45.72 54.61) (width 1) (layer B.Cu) (net 2) (status 10))
  (segment (start 45.72 54.61) (end 29.21 54.61) (width 1) (layer B.Cu) (net 2))
  (segment (start 66.04 58.42) (end 66.04 54.61) (width 1) (layer B.Cu) (net 2) (status 10))
  (segment (start 66.04 54.61) (end 45.72 54.61) (width 1) (layer B.Cu) (net 2))
  (segment (start 83.82 58.42) (end 83.82 54.61) (width 1) (layer B.Cu) (net 2) (status 10))
  (segment (start 83.82 54.61) (end 66.04 54.61) (width 1) (layer B.Cu) (net 2))
  (segment (start 101.6 58.42) (end 101.6 54.61) (width 1) (layer B.Cu) (net 2) (status 10))
  (segment (start 101.6 54.61) (end 83.82 54.61) (width 1) (layer B.Cu) (net 2))
  (segment (start 119.38 58.42) (end 119.38 54.61) (width 1) (layer B.Cu) (net 2) (status 10))
  (segment (start 119.38 54.61) (end 101.6 54.61) (width 1) (layer B.Cu) (net 2))
  (segment (start 137.16 58.42) (end 137.16 54.61) (width 1) (layer B.Cu) (net 2) (status 10))
  (segment (start 137.16 54.61) (end 119.38 54.61) (width 1) (layer B.Cu) (net 2))
  (segment (start 167.64 54.61) (end 137.16 54.61) (width 1) (layer B.Cu) (net 2))
  (segment (start 154.94 56.52) (end 154.94 54.61) (width 1) (layer B.Cu) (net 2))
  (segment (start 154.94 58.42) (end 154.94 56.52) (width 1) (layer B.Cu) (net 2) (status 10))
  (segment (start 170.18 55.88) (end 168.91 54.61) (width 1) (layer B.Cu) (net 2))
  (segment (start 168.91 54.61) (end 167.64 54.61) (width 1) (layer B.Cu) (net 2))
  (segment (start 137.16 55.28) (end 136.49 54.61) (width 1) (layer F.Cu) (net 2) (status 20))
  (segment (start 137.16 58.42) (end 137.16 55.28) (width 1) (layer F.Cu) (net 2) (status 10))
  (segment (start 172.72 73.66) (end 170.18 73.66) (width 1) (layer B.Cu) (net 2))
  (segment (start 91.44 55.28) (end 92.11 54.61) (width 1) (layer F.Cu) (net 3) (status 20))
  (segment (start 91.44 58.42) (end 91.44 55.28) (width 1) (layer F.Cu) (net 3) (status 10))
  (segment (start 157.48 71.12) (end 157.48 73.66) (width 0.5) (layer B.Cu) (net 3) (status 20))
  (segment (start 91.44 62.23) (end 93.98 64.77) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 93.98 64.77) (end 151.13 64.77) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 151.13 64.77) (end 157.48 71.12) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 91.44 62.23) (end 91.44 58.42) (width 0.5) (layer B.Cu) (net 3) (status 20))
  (segment (start 165.1 71.12) (end 165.1 73.66) (width 0.5) (layer B.Cu) (net 4) (status 20))
  (segment (start 144.78 59.69) (end 146.05 60.96) (width 0.5) (layer B.Cu) (net 4))
  (segment (start 146.05 60.96) (end 154.94 60.96) (width 0.5) (layer B.Cu) (net 4))
  (segment (start 154.94 60.96) (end 165.1 71.12) (width 0.5) (layer B.Cu) (net 4))
  (segment (start 144.78 59.69) (end 144.78 58.42) (width 0.5) (layer B.Cu) (net 4) (status 20))
  (segment (start 144.78 55.88) (end 146.05 54.61) (width 1) (layer F.Cu) (net 4) (status 20))
  (segment (start 144.78 58.42) (end 144.78 55.88) (width 1) (layer F.Cu) (net 4) (status 10))
  (segment (start 73.66 55.58) (end 74.63 54.61) (width 1) (layer F.Cu) (net 5) (status 20))
  (segment (start 73.66 58.42) (end 73.66 55.58) (width 1) (layer F.Cu) (net 5) (status 10))
  (segment (start 73.66 63.5) (end 76.2 66.04) (width 0.5) (layer B.Cu) (net 5))
  (segment (start 154.94 71.12) (end 154.94 73.66) (width 0.5) (layer B.Cu) (net 5) (status 20))
  (segment (start 76.2 66.04) (end 149.86 66.04) (width 0.5) (layer B.Cu) (net 5))
  (segment (start 149.86 66.04) (end 154.94 71.12) (width 0.5) (layer B.Cu) (net 5))
  (segment (start 73.66 63.5) (end 73.66 58.42) (width 0.5) (layer B.Cu) (net 5) (status 20))
  (segment (start 127 55.58) (end 127.97 54.61) (width 1) (layer F.Cu) (net 6) (status 20))
  (segment (start 127 58.42) (end 127 55.58) (width 1) (layer F.Cu) (net 6) (status 10))
  (segment (start 162.56 71.12) (end 162.56 73.66) (width 0.5) (layer B.Cu) (net 6) (status 20))
  (segment (start 128.27 62.23) (end 153.67 62.23) (width 0.5) (layer B.Cu) (net 6))
  (segment (start 153.67 62.23) (end 162.56 71.12) (width 0.5) (layer B.Cu) (net 6))
  (segment (start 128.27 62.23) (end 127 60.96) (width 0.5) (layer B.Cu) (net 6))
  (segment (start 127 60.96) (end 127 58.42) (width 0.5) (layer B.Cu) (net 6) (status 20))
  (segment (start 53.34 55.58) (end 54.31 54.61) (width 1) (layer F.Cu) (net 7) (status 20))
  (segment (start 53.34 58.42) (end 53.34 55.58) (width 1) (layer F.Cu) (net 7) (status 10))
  (segment (start 152.4 71.12) (end 152.4 73.66) (width 0.5) (layer B.Cu) (net 7) (status 20))
  (segment (start 53.34 64.77) (end 55.88 67.31) (width 0.5) (layer B.Cu) (net 7))
  (segment (start 148.59 67.31) (end 152.4 71.12) (width 0.5) (layer B.Cu) (net 7))
  (segment (start 55.88 67.31) (end 148.59 67.31) (width 0.5) (layer B.Cu) (net 7))
  (segment (start 53.34 64.77) (end 53.34 58.42) (width 0.5) (layer B.Cu) (net 7) (status 20))
  (segment (start 109.22 55.48) (end 110.09 54.61) (width 1) (layer F.Cu) (net 8) (status 20))
  (segment (start 109.22 58.42) (end 109.22 55.48) (width 1) (layer F.Cu) (net 8) (status 10))
  (segment (start 160.02 71.12) (end 160.02 73.66) (width 0.5) (layer B.Cu) (net 8) (status 20))
  (segment (start 109.22 60.96) (end 111.76 63.5) (width 0.5) (layer B.Cu) (net 8))
  (segment (start 111.76 63.5) (end 152.4 63.5) (width 0.5) (layer B.Cu) (net 8))
  (segment (start 152.4 63.5) (end 160.02 71.12) (width 0.5) (layer B.Cu) (net 8))
  (segment (start 109.22 60.96) (end 109.22 58.42) (width 0.5) (layer B.Cu) (net 8) (status 20))
  (segment (start 35.56 55.28) (end 36.23 54.61) (width 1) (layer F.Cu) (net 9) (status 20))
  (segment (start 35.56 58.42) (end 35.56 55.28) (width 1) (layer F.Cu) (net 9) (status 10))
  (segment (start 149.86 72.31) (end 146.13 68.58) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 149.86 73.66) (end 149.86 72.31) (width 0.5) (layer B.Cu) (net 9) (status 10))
  (segment (start 146.13 68.58) (end 38.1 68.58) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 38.1 68.58) (end 35.56 66.04) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 35.56 66.04) (end 35.56 58.42) (width 0.5) (layer B.Cu) (net 9) (status 20))
  (via (at 174.625 34.29) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 10))
  (via (at 174.625 53.34) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 10))
  (via (at 40.64 15.875) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 10))
  (via (at 78.74 15.875) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 10))
  (via (at 96.52 15.875) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 10))
  (via (at 114.3 15.875) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 10))
  (via (at 132.08 15.875) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 10))
  (via (at 150.495 15.875) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 10))
  (via (at 144.145 76.2) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 10))
  (via (at 36.83 76.835) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 10))
  (via (at 17.145 65.405) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 10))
  (via (at 17.78 41.91) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 10) (tstamp 5CE6B2D7))
  (segment (start 166.97 49.53) (end 164.5 49.53) (width 1) (layer F.Cu) (net 11) (status 20))
  (segment (start 167.470001 50.030001) (end 166.97 49.53) (width 1) (layer F.Cu) (net 11))
  (segment (start 165.1 67.31) (end 167.470001 64.939999) (width 1) (layer F.Cu) (net 11))
  (segment (start 167.470001 50.030001) (end 167.470001 64.939999) (width 1) (layer F.Cu) (net 11))
  (segment (start 165.1 67.31) (end 139.065 67.31) (width 1) (layer F.Cu) (net 11))
  (segment (start 134.091999 75.448001) (end 134.091999 73.553001) (width 1) (layer F.Cu) (net 11))
  (segment (start 133.33 76.21) (end 134.091999 75.448001) (width 1) (layer F.Cu) (net 11) (status 10))
  (segment (start 134.091999 73.553001) (end 136.525 71.12) (width 1) (layer F.Cu) (net 11))
  (segment (start 136.525 69.85) (end 139.065 67.31) (width 1) (layer F.Cu) (net 11))
  (segment (start 136.525 71.12) (end 136.525 69.85) (width 1) (layer F.Cu) (net 11))
  (segment (start 152.47 49.53) (end 154.94 49.53) (width 1) (layer F.Cu) (net 12) (status 20))
  (segment (start 151.020011 50.979989) (end 152.47 49.53) (width 1) (layer F.Cu) (net 12))
  (segment (start 128.23 76.21) (end 130.81 73.63) (width 1) (layer F.Cu) (net 12) (status 10))
  (segment (start 146.620433 65.50001) (end 151.020011 61.100431) (width 1) (layer F.Cu) (net 12))
  (segment (start 151.020011 61.100431) (end 151.020011 50.979989) (width 1) (layer F.Cu) (net 12))
  (segment (start 146.620433 65.50001) (end 137.69999 65.50001) (width 1) (layer F.Cu) (net 12))
  (segment (start 137.69999 65.50001) (end 135.255 67.945) (width 1) (layer F.Cu) (net 12))
  (segment (start 130.81 70.282238) (end 130.81 73.63) (width 1) (layer F.Cu) (net 12))
  (segment (start 133.147238 67.945) (end 130.81 70.282238) (width 1) (layer F.Cu) (net 12))
  (segment (start 135.255 67.945) (end 133.147238 67.945) (width 1) (layer F.Cu) (net 12))
  (segment (start 26.67 46.99) (end 25.7 46.99) (width 1) (layer F.Cu) (net 13) (tstamp 5CD30EAD) (status 30))
  (segment (start 17.78 20.32) (end 30.48 20.32) (width 1.5) (layer B.Cu) (net 13) (status 10))
  (segment (start 17.78 22.86) (end 163.83 22.86) (width 1.5) (layer B.Cu) (net 13) (status 10))
  (segment (start 17.78 25.4) (end 30.48 25.4) (width 1.5) (layer B.Cu) (net 13) (status 10))
  (segment (start 17.78 27.94) (end 30.48 27.94) (width 1.5) (layer B.Cu) (net 13) (status 10))
  (segment (start 17.78 30.48) (end 30.48 30.48) (width 1.5) (layer B.Cu) (net 13) (status 10))
  (segment (start 17.78 33.02) (end 30.48 33.02) (width 1.5) (layer B.Cu) (net 13) (status 10))
  (segment (start 17.78 35.56) (end 30.48 35.56) (width 1.5) (layer B.Cu) (net 13) (status 10))
  (segment (start 17.78 38.1) (end 163.83 38.1) (width 1.5) (layer B.Cu) (net 13) (status 10))
  (segment (start 30.48 20.32) (end 163.83 20.32) (width 1.5) (layer B.Cu) (net 13) (tstamp 5CD498BC))
  (segment (start 30.48 35.56) (end 33.02 35.56) (width 1.5) (layer B.Cu) (net 13) (tstamp 5CD498D9))
  (segment (start 30.48 33.02) (end 33.02 33.02) (width 1.5) (layer B.Cu) (net 13) (tstamp 5CD498DB))
  (segment (start 30.48 30.48) (end 163.83 30.48) (width 1.5) (layer B.Cu) (net 13) (tstamp 5CD498DD))
  (segment (start 33.02 27.94) (end 163.83 27.94) (width 1.5) (layer B.Cu) (net 13) (tstamp 5CD498E1))
  (segment (start 30.48 27.94) (end 33.02 27.94) (width 1.5) (layer B.Cu) (net 13) (tstamp 5CD498E3))
  (segment (start 30.48 25.4) (end 163.83 25.4) (width 1.5) (layer B.Cu) (net 13) (tstamp 5CD498E5))
  (segment (start 33.02 35.56) (end 163.83 35.56) (width 1.5) (layer B.Cu) (net 13) (tstamp 5CD498F7))
  (segment (start 33.02 33.02) (end 163.83 33.02) (width 1.5) (layer B.Cu) (net 13) (tstamp 5CD498F9))
  (segment (start 25.809998 40.64) (end 27.94 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 26.67 46.99) (end 24.2 46.99) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 27.94 40.64) (end 27.94 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 24.2 46.99) (end 23.699999 46.489999) (width 1) (layer F.Cu) (net 13))
  (segment (start 23.699999 46.489999) (end 23.699999 42.749999) (width 1) (layer F.Cu) (net 13))
  (segment (start 23.699999 42.749999) (end 25.809998 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 30.48 50.73) (end 30.48 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 29.14 52.07) (end 30.48 50.73) (width 1) (layer F.Cu) (net 13))
  (segment (start 26.67 52.07) (end 29.14 52.07) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 33.76 52.07) (end 33.02 51.33) (width 1) (layer F.Cu) (net 13))
  (segment (start 33.02 51.33) (end 33.02 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 36.23 52.07) (end 33.76 52.07) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 38.1 40.64) (end 35.56 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 36.23 46.99) (end 38.7 46.99) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 35.56 40.64) (end 35.56 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 38.7 46.99) (end 39.200001 46.489999) (width 1) (layer F.Cu) (net 13))
  (segment (start 39.200001 46.489999) (end 39.200001 41.740001) (width 1) (layer F.Cu) (net 13))
  (segment (start 39.200001 41.740001) (end 38.1 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 43.18 40.64) (end 45.72 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 44.75 46.99) (end 42.28 46.99) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 42.28 46.99) (end 41.779999 46.489999) (width 1) (layer F.Cu) (net 13))
  (segment (start 41.779999 46.489999) (end 41.779999 42.040001) (width 1) (layer F.Cu) (net 13))
  (segment (start 41.779999 42.040001) (end 43.18 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 47.22 52.07) (end 48.26 51.03) (width 1) (layer F.Cu) (net 13))
  (segment (start 44.75 52.07) (end 47.22 52.07) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 51.84 52.07) (end 50.8 51.03) (width 1) (layer F.Cu) (net 13))
  (segment (start 54.31 52.07) (end 51.84 52.07) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 55.88 40.64) (end 53.34 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 54.31 46.99) (end 56.440002 46.99) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 56.440002 46.99) (end 57.280001 46.150001) (width 1) (layer F.Cu) (net 13))
  (segment (start 57.280001 42.040001) (end 55.88 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 57.280001 46.150001) (end 57.280001 42.040001) (width 1) (layer F.Cu) (net 13))
  (segment (start 64.209998 40.64) (end 66.04 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 65.07 46.99) (end 62.6 46.99) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 62.099999 42.749999) (end 64.209998 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 62.099999 46.489999) (end 62.099999 42.749999) (width 1) (layer F.Cu) (net 13))
  (segment (start 62.6 46.99) (end 62.099999 46.489999) (width 1) (layer F.Cu) (net 13))
  (segment (start 67.54 52.07) (end 68.58 51.03) (width 1) (layer F.Cu) (net 13))
  (segment (start 65.07 52.07) (end 67.54 52.07) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 72.499998 52.07) (end 71.12 50.690002) (width 1) (layer F.Cu) (net 13))
  (segment (start 74.63 52.07) (end 72.499998 52.07) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 75.490002 40.64) (end 73.66 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 74.63 46.99) (end 77.1 46.99) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 77.1 46.99) (end 77.600001 46.489999) (width 1) (layer F.Cu) (net 13))
  (segment (start 77.600001 46.489999) (end 77.600001 42.749999) (width 1) (layer F.Cu) (net 13))
  (segment (start 77.600001 42.749999) (end 75.490002 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 82.55 46.99) (end 80.08 46.99) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 80.08 46.99) (end 79.579999 46.489999) (width 1) (layer F.Cu) (net 13))
  (segment (start 79.579999 46.489999) (end 79.579999 42.749999) (width 1) (layer F.Cu) (net 13))
  (segment (start 81.689998 40.64) (end 83.82 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 79.579999 42.749999) (end 81.689998 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 85.02 52.07) (end 86.36 50.73) (width 1) (layer F.Cu) (net 13))
  (segment (start 82.55 52.07) (end 85.02 52.07) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 89.979998 52.07) (end 88.9 50.990002) (width 1) (layer F.Cu) (net 13))
  (segment (start 92.11 52.07) (end 89.979998 52.07) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 92.970002 40.64) (end 91.44 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 92.11 46.99) (end 94.58 46.99) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 94.58 46.99) (end 95.080001 46.489999) (width 1) (layer F.Cu) (net 13))
  (segment (start 95.080001 46.489999) (end 95.080001 42.749999) (width 1) (layer F.Cu) (net 13))
  (segment (start 95.080001 42.749999) (end 92.970002 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 100.53 46.99) (end 98.399998 46.99) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 98.399998 46.99) (end 97.559999 46.150001) (width 1) (layer F.Cu) (net 13))
  (segment (start 99.06 40.64) (end 101.6 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 97.559999 46.150001) (end 97.559999 42.140001) (width 1) (layer F.Cu) (net 13))
  (segment (start 97.559999 42.140001) (end 99.06 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 103 52.07) (end 104.14 50.93) (width 1) (layer F.Cu) (net 13))
  (segment (start 100.53 52.07) (end 103 52.07) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 107.959998 52.07) (end 106.68 50.790002) (width 1) (layer F.Cu) (net 13))
  (segment (start 110.09 52.07) (end 107.959998 52.07) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 110.950002 40.64) (end 109.22 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 110.09 46.99) (end 112.56 46.99) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 112.56 46.99) (end 113.060001 46.489999) (width 1) (layer F.Cu) (net 13))
  (segment (start 113.060001 46.489999) (end 113.060001 42.749999) (width 1) (layer F.Cu) (net 13))
  (segment (start 113.060001 42.749999) (end 110.950002 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 118.41 46.99) (end 115.94 46.99) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 117.549998 40.64) (end 119.38 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 115.439999 42.749999) (end 117.549998 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 115.439999 46.489999) (end 115.439999 42.749999) (width 1) (layer F.Cu) (net 13))
  (segment (start 115.94 46.99) (end 115.439999 46.489999) (width 1) (layer F.Cu) (net 13))
  (segment (start 120.88 52.07) (end 121.92 51.03) (width 1) (layer F.Cu) (net 13))
  (segment (start 118.41 52.07) (end 120.88 52.07) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 125.5 52.07) (end 124.46 51.03) (width 1) (layer F.Cu) (net 13))
  (segment (start 127.97 52.07) (end 125.5 52.07) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 127.97 46.99) (end 130.100002 46.99) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 130.100002 46.99) (end 130.940001 46.150001) (width 1) (layer F.Cu) (net 13))
  (segment (start 128.830002 40.64) (end 127 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 130.940001 46.150001) (end 130.940001 42.749999) (width 1) (layer F.Cu) (net 13))
  (segment (start 130.940001 42.749999) (end 128.830002 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 135.629998 40.64) (end 137.16 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 136.49 46.99) (end 134.02 46.99) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 134.02 46.99) (end 133.519999 46.489999) (width 1) (layer F.Cu) (net 13))
  (segment (start 133.519999 46.489999) (end 133.519999 42.749999) (width 1) (layer F.Cu) (net 13))
  (segment (start 133.519999 42.749999) (end 135.629998 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 138.96 52.07) (end 139.7 51.33) (width 1) (layer F.Cu) (net 13))
  (segment (start 136.49 52.07) (end 138.96 52.07) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 143.58 52.07) (end 142.24 50.73) (width 1) (layer F.Cu) (net 13))
  (segment (start 146.05 52.07) (end 143.58 52.07) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 146.05 46.99) (end 148.52 46.99) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 148.52 46.99) (end 149.020001 46.489999) (width 1) (layer F.Cu) (net 13))
  (segment (start 146.910002 40.64) (end 144.78 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 149.020001 46.489999) (end 149.020001 42.749999) (width 1) (layer F.Cu) (net 13))
  (segment (start 149.020001 42.749999) (end 146.910002 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 154.079998 40.64) (end 156.21 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 154.94 46.99) (end 152.47 46.99) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 152.47 46.99) (end 151.969999 46.489999) (width 1) (layer F.Cu) (net 13))
  (segment (start 151.969999 46.489999) (end 151.969999 42.749999) (width 1) (layer F.Cu) (net 13))
  (segment (start 151.969999 42.749999) (end 154.079998 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 157.41 52.07) (end 158.75 50.73) (width 1) (layer F.Cu) (net 13))
  (segment (start 154.94 52.07) (end 157.41 52.07) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 162.03 52.07) (end 161.29 51.33) (width 1) (layer F.Cu) (net 13))
  (segment (start 164.5 52.07) (end 162.03 52.07) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 165.360002 40.64) (end 163.83 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 164.5 46.99) (end 166.97 46.99) (width 1) (layer F.Cu) (net 13) (status 10))
  (segment (start 166.97 46.99) (end 167.470001 46.489999) (width 1) (layer F.Cu) (net 13))
  (segment (start 167.470001 46.489999) (end 167.470001 42.749999) (width 1) (layer F.Cu) (net 13))
  (segment (start 167.470001 42.749999) (end 165.360002 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 45.72 40.64) (end 45.72 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 53.34 40.64) (end 53.34 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 48.26 51.03) (end 48.26 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 50.8 51.03) (end 50.8 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 66.04 40.64) (end 66.04 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 68.58 51.03) (end 68.58 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 71.12 50.690002) (end 71.12 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 73.66 40.64) (end 73.66 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 83.82 40.64) (end 83.82 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 86.36 50.73) (end 86.36 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 88.9 50.990002) (end 88.9 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 91.44 40.64) (end 91.44 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 101.6 40.64) (end 101.6 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 104.14 50.93) (end 104.14 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 106.68 50.790002) (end 106.68 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 109.22 40.64) (end 109.22 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 119.38 40.64) (end 119.38 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 121.92 40.64) (end 121.92 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 121.92 51.03) (end 121.92 40.64) (width 1) (layer F.Cu) (net 13))
  (segment (start 124.46 51.03) (end 124.46 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 127 40.64) (end 127 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 137.16 40.64) (end 137.16 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 139.7 51.33) (end 139.7 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 142.24 50.73) (end 142.24 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 144.78 40.64) (end 144.78 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 156.21 40.64) (end 156.21 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 163.83 40.64) (end 163.83 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 158.75 50.73) (end 158.75 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 161.29 51.33) (end 161.29 38.1) (width 1) (layer F.Cu) (net 13))
  (segment (start 156.21 38.1) (end 156.21 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 144.78 38.1) (end 144.78 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 142.24 38.1) (end 142.24 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 139.7 38.1) (end 139.7 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 137.16 38.1) (end 137.16 30.48) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 137.16 30.48) (end 137.16 20.32) (width 1.5) (layer F.Cu) (net 13))
  (via (at 104.14 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B2D))
  (via (at 101.6 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B2C))
  (via (at 101.6 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B2B))
  (via (at 104.14 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B2A))
  (via (at 106.68 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B29))
  (via (at 101.6 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B28))
  (via (at 104.14 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B27))
  (via (at 101.6 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B26))
  (via (at 101.6 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B24))
  (via (at 109.22 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B23))
  (via (at 101.6 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B22))
  (via (at 109.22 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B21))
  (via (at 106.68 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B20))
  (via (at 101.6 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B1F))
  (via (at 101.6 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B1E))
  (via (at 83.82 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AFA))
  (via (at 86.36 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AF9))
  (via (at 86.36 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AF8))
  (via (at 91.44 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AF7))
  (segment (start 35.56 22.86) (end 35.56 20.32) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498C2))
  (via (at 35.56 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 33.02 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 30.48 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 30.48 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 30.48 22.86) (end 30.48 20.32) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498BA))
  (via (at 27.94 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 27.94 22.86) (end 27.94 20.32) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498B8))
  (via (at 73.66 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A9C))
  (via (at 66.04 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A9B))
  (via (at 68.58 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A9A))
  (via (at 73.66 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A99))
  (via (at 66.04 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A98))
  (via (at 71.12 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A97))
  (via (at 73.66 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A96))
  (via (at 68.58 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A95))
  (via (at 66.04 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A94))
  (via (at 124.46 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B6A))
  (via (at 119.38 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B69))
  (via (at 121.92 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B67))
  (via (at 127 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B66))
  (via (at 127 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B65))
  (via (at 127 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B64))
  (via (at 106.68 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B40))
  (via (at 106.68 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B3F))
  (via (at 106.68 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B3E))
  (via (at 104.14 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B3D))
  (via (at 106.68 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B3C))
  (via (at 104.14 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B3B))
  (via (at 91.44 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49ADA))
  (via (at 86.36 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AD9))
  (via (at 83.82 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AD8))
  (via (at 71.12 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AB4))
  (via (at 71.12 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AB2))
  (via (at 124.46 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B77))
  (via (at 127 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B76))
  (via (at 127 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B75))
  (via (at 127 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B74))
  (via (at 121.92 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B73))
  (via (at 127 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B72))
  (via (at 119.38 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B71))
  (via (at 121.92 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B70))
  (via (at 124.46 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B6F))
  (via (at 121.92 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B6E))
  (via (at 121.92 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B6D))
  (via (at 124.46 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B6C))
  (via (at 121.92 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B6B))
  (segment (start 127 38.1) (end 127 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 124.46 38.1) (end 124.46 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 121.92 38.1) (end 121.92 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 119.38 38.1) (end 119.38 27.94) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 119.38 27.94) (end 119.38 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 109.22 38.1) (end 109.22 20.32) (width 1.5) (layer F.Cu) (net 13))
  (via (at 161.29 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BF8))
  (via (at 158.75 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BF7))
  (via (at 156.21 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BF6))
  (via (at 163.83 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BF5))
  (via (at 161.29 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BF4))
  (via (at 161.29 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BF3))
  (via (at 156.21 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BF2))
  (via (at 158.75 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BF1))
  (via (at 144.78 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BCC))
  (via (at 144.78 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BCB))
  (via (at 137.16 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BCA))
  (via (at 137.16 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BC9))
  (via (at 124.46 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B84))
  (via (at 119.38 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B83))
  (via (at 127 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B82))
  (via (at 124.46 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B80))
  (via (at 119.38 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B7F))
  (via (at 119.38 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B7E))
  (via (at 121.92 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B7C))
  (via (at 119.38 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B7B))
  (via (at 119.38 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B7A))
  (via (at 121.92 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B79))
  (via (at 119.38 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B78))
  (segment (start 158.75 38.1) (end 158.75 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 161.29 38.1) (end 161.29 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 163.83 38.1) (end 163.83 20.32) (width 1.5) (layer F.Cu) (net 13))
  (via (at 158.75 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C11))
  (via (at 163.83 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C10))
  (via (at 156.21 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C0F))
  (via (at 158.75 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C0E))
  (via (at 158.75 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C0D))
  (via (at 161.29 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C0C))
  (via (at 156.21 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C0B))
  (via (at 158.75 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C0A))
  (via (at 161.29 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C09))
  (via (at 163.83 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C08))
  (via (at 156.21 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C07))
  (via (at 161.29 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C06))
  (via (at 33.02 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 33.02 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 33.02 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 33.02 38.1) (end 33.02 30.48) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498F5))
  (via (at 35.56 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 27.94 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 27.94 27.94) (end 27.94 25.4) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498CD))
  (via (at 27.94 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 27.94 25.4) (end 27.94 22.86) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498CB))
  (via (at 33.02 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 33.02 22.86) (end 33.02 20.32) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498C4))
  (via (at 35.56 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 50.8 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A0E))
  (via (at 53.34 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A0D))
  (via (at 48.26 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A0C))
  (via (at 53.34 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A0B))
  (via (at 50.8 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A0A))
  (via (at 48.26 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A06))
  (via (at 45.72 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A05))
  (via (at 45.72 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A03))
  (via (at 53.34 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A02))
  (segment (start 27.94 38.1) (end 27.94 35.56) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498D5))
  (via (at 27.94 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 27.94 35.56) (end 27.94 33.02) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498D3))
  (via (at 27.94 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 27.94 33.02) (end 27.94 30.48) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498D1))
  (via (at 27.94 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 27.94 30.48) (end 27.94 27.94) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498CF))
  (segment (start 35.56 38.1) (end 35.56 35.56) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498F3))
  (via (at 35.56 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 35.56 35.56) (end 35.56 33.02) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498F1))
  (via (at 35.56 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 35.56 33.02) (end 35.56 30.48) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498EF))
  (via (at 35.56 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 35.56 30.48) (end 35.56 27.94) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498ED))
  (via (at 35.56 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 142.24 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BBB))
  (via (at 142.24 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BBA))
  (via (at 144.78 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BB8))
  (via (at 137.16 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BB7))
  (via (at 139.7 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BB6))
  (via (at 142.24 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BB5))
  (segment (start 35.56 27.94) (end 35.56 25.4) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498EB))
  (via (at 35.56 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 35.56 25.4) (end 35.56 22.86) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498E9))
  (via (at 33.02 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 33.02 25.4) (end 33.02 22.86) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498E7))
  (via (at 30.48 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 45.72 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A01))
  (via (at 48.26 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A00))
  (via (at 50.8 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD499FF))
  (via (at 53.34 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD499FC))
  (via (at 50.8 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD499FB))
  (via (at 48.26 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD499FA))
  (via (at 45.72 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD499F5))
  (via (at 45.72 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD499F4))
  (via (at 30.48 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 33.02 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 33.02 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 33.02 30.48) (end 33.02 25.4) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498DF))
  (via (at 30.48 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 163.83 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C12))
  (via (at 30.48 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 30.48 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 30.48 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (segment (start 30.48 38.1) (end 30.48 22.86) (width 1.5) (layer F.Cu) (net 13) (tstamp 5CD498D7))
  (via (at 27.94 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 48.26 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD499F3))
  (via (at 48.26 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD499F2))
  (via (at 45.72 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD499F1))
  (via (at 53.34 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD499ED))
  (via (at 50.8 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD499EA))
  (via (at 53.34 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD499E8))
  (via (at 53.34 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD499E6))
  (via (at 45.72 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD499E5))
  (via (at 48.26 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD499E4))
  (segment (start 68.58 38.1) (end 68.58 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 66.04 38.1) (end 66.04 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 50.8 38.1) (end 50.8 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 48.26 38.1) (end 48.26 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 53.34 38.1) (end 53.34 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 45.72 38.1) (end 45.72 20.32) (width 1.5) (layer F.Cu) (net 13))
  (via (at 91.44 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AEB))
  (via (at 83.82 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AEA))
  (via (at 83.82 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AE9))
  (via (at 88.9 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AE8))
  (via (at 88.9 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AE6))
  (via (at 88.9 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AE5))
  (via (at 91.44 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AE4))
  (via (at 88.9 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AE3))
  (via (at 91.44 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AE2))
  (via (at 66.04 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AAD))
  (via (at 68.58 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AAC))
  (via (at 66.04 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AAB))
  (via (at 66.04 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AAA))
  (via (at 68.58 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AA9))
  (via (at 66.04 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AA8))
  (via (at 68.58 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AA7))
  (via (at 71.12 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AA6))
  (segment (start 88.9 27.94) (end 88.9 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 86.36 38.1) (end 86.36 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 83.82 38.1) (end 83.82 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 73.66 38.1) (end 73.66 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 71.12 38.1) (end 71.12 27.94) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 71.12 27.94) (end 71.12 20.32) (width 1.5) (layer F.Cu) (net 13))
  (via (at 109.22 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B3A))
  (via (at 104.14 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B39))
  (via (at 106.68 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B38))
  (via (at 104.14 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B36))
  (via (at 109.22 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B35))
  (via (at 109.22 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B34))
  (via (at 106.68 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B33))
  (via (at 104.14 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B32))
  (via (at 109.22 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B31))
  (via (at 109.22 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B2F))
  (via (at 109.22 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B2E))
  (via (at 163.83 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C05))
  (via (at 156.21 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C04))
  (via (at 161.29 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C02))
  (via (at 158.75 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C01))
  (via (at 156.21 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49C00))
  (via (at 161.29 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BFF))
  (via (at 163.83 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BFE))
  (via (at 156.21 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BFD))
  (via (at 163.83 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BFC))
  (via (at 158.75 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BFB))
  (via (at 163.83 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BF9))
  (via (at 91.44 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AF6))
  (via (at 86.36 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AF5))
  (via (at 88.9 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AF4))
  (via (at 86.36 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AF3))
  (via (at 83.82 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AF2))
  (via (at 83.82 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AF1))
  (via (at 86.36 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AF0))
  (via (at 88.9 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AEF))
  (via (at 91.44 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AEE))
  (via (at 88.9 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AED))
  (via (at 73.66 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AA4))
  (via (at 68.58 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AA3))
  (via (at 71.12 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AA2))
  (via (at 71.12 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AA1))
  (via (at 73.66 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AA0))
  (via (at 73.66 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A9F))
  (via (at 71.12 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A9E))
  (via (at 68.58 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A9D))
  (via (at 83.82 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AE1))
  (via (at 86.36 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AE0))
  (via (at 91.44 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49ADF))
  (via (at 83.82 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49ADE))
  (via (at 88.9 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49ADC))
  (via (at 86.36 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49ADB))
  (via (at 71.12 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AB0))
  (via (at 73.66 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AAF))
  (via (at 73.66 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49AAE))
  (via (at 27.94 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13))
  (via (at 139.7 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BB4))
  (via (at 144.78 38.1) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BB3))
  (via (at 139.7 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BB2))
  (via (at 142.24 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BB1))
  (via (at 144.78 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BB0))
  (via (at 139.7 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BAE))
  (via (at 137.16 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BAD))
  (via (at 137.16 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BAC))
  (via (at 142.24 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BAB))
  (via (at 139.7 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BAA))
  (via (at 124.46 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B86))
  (via (at 124.46 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49B85))
  (segment (start 106.68 38.1) (end 106.68 30.48) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 106.68 30.48) (end 106.68 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 104.14 38.1) (end 104.14 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 101.6 38.1) (end 101.6 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 91.44 38.1) (end 91.44 20.32) (width 1.5) (layer F.Cu) (net 13))
  (segment (start 88.9 38.1) (end 88.9 27.94) (width 1.5) (layer F.Cu) (net 13))
  (via (at 68.58 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A93))
  (via (at 66.04 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A92))
  (via (at 50.8 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A1C))
  (via (at 50.8 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A18))
  (via (at 50.8 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A16))
  (via (at 53.34 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A15))
  (via (at 45.72 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A14))
  (via (at 48.26 30.48) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49A13))
  (via (at 142.24 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BC7))
  (via (at 139.7 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BC6))
  (via (at 144.78 25.4) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BC5))
  (via (at 139.7 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BC4))
  (via (at 137.16 22.86) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BC3))
  (via (at 142.24 27.94) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BC2))
  (via (at 142.24 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BC1))
  (via (at 144.78 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BC0))
  (via (at 137.16 20.32) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BBF))
  (via (at 144.78 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BBE))
  (via (at 137.16 33.02) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BBD))
  (via (at 139.7 35.56) (size 1) (drill 0.8) (layers F.Cu B.Cu) (net 13) (tstamp 5CD49BBC))
  (segment (start 94.58 49.53) (end 92.11 49.53) (width 1) (layer F.Cu) (net 14) (status 20))
  (segment (start 95.080001 50.030001) (end 94.58 49.53) (width 1) (layer F.Cu) (net 14))
  (segment (start 95.06 50.050002) (end 95.080001 50.030001) (width 1) (layer F.Cu) (net 14))
  (segment (start 92.53 76.21) (end 95.25 73.49) (width 1) (layer F.Cu) (net 14) (status 10))
  (segment (start 95.25 50.2) (end 95.080001 50.030001) (width 1) (layer F.Cu) (net 14))
  (segment (start 95.25 73.49) (end 95.25 50.2) (width 1) (layer F.Cu) (net 14))
  (segment (start 80.08 49.53) (end 82.55 49.53) (width 1) (layer F.Cu) (net 15) (status 20))
  (segment (start 79.47001 50.13999) (end 80.08 49.53) (width 1) (layer F.Cu) (net 15))
  (segment (start 87.43 76.21) (end 86.668001 75.448001) (width 1) (layer F.Cu) (net 15) (status 10))
  (segment (start 84.836 68.516) (end 79.47001 63.15001) (width 1) (layer F.Cu) (net 15))
  (segment (start 86.116001 75.448001) (end 84.836 74.168) (width 1) (layer F.Cu) (net 15))
  (segment (start 86.668001 75.448001) (end 86.116001 75.448001) (width 1) (layer F.Cu) (net 15))
  (segment (start 79.47001 63.15001) (end 79.47001 50.13999) (width 1) (layer F.Cu) (net 15))
  (segment (start 84.836 74.168) (end 84.836 68.516) (width 1) (layer F.Cu) (net 15))
  (segment (start 149.020001 50.030001) (end 148.52 49.53) (width 1) (layer F.Cu) (net 16))
  (segment (start 149.020001 60.272001) (end 149.020001 50.030001) (width 1) (layer F.Cu) (net 16))
  (segment (start 145.792002 63.5) (end 149.020001 60.272001) (width 1) (layer F.Cu) (net 16))
  (segment (start 125.73 73.61) (end 125.73 68.58) (width 1) (layer F.Cu) (net 16))
  (segment (start 148.52 49.53) (end 146.05 49.53) (width 1) (layer F.Cu) (net 16) (status 20))
  (segment (start 123.13 76.21) (end 125.73 73.61) (width 1) (layer F.Cu) (net 16) (status 10))
  (segment (start 145.792002 63.5) (end 134.62 63.5) (width 1) (layer F.Cu) (net 16))
  (segment (start 134.62 63.5) (end 130.175 67.945) (width 1) (layer F.Cu) (net 16))
  (segment (start 126.365 67.945) (end 125.73 68.58) (width 1) (layer F.Cu) (net 16))
  (segment (start 130.175 67.945) (end 126.365 67.945) (width 1) (layer F.Cu) (net 16))
  (segment (start 129.54 65.751559) (end 124.113441 65.751559) (width 1) (layer F.Cu) (net 17))
  (segment (start 136.49 49.53) (end 134.02 49.53) (width 1) (layer F.Cu) (net 17) (status 10))
  (segment (start 124.113441 65.751559) (end 120.65 69.215) (width 1) (layer F.Cu) (net 17))
  (segment (start 134.02 49.53) (end 132.940011 50.609989) (width 1) (layer F.Cu) (net 17))
  (segment (start 120.65 69.215) (end 120.65 73.59) (width 1) (layer F.Cu) (net 17))
  (segment (start 132.940011 50.609989) (end 132.940011 62.351548) (width 1) (layer F.Cu) (net 17))
  (segment (start 120.65 73.59) (end 118.03 76.21) (width 1) (layer F.Cu) (net 17) (status 20))
  (segment (start 132.940011 62.351548) (end 129.54 65.751559) (width 1) (layer F.Cu) (net 17))
  (segment (start 65.07 49.53) (end 62.6 49.53) (width 1) (layer F.Cu) (net 18) (status 10))
  (segment (start 62.6 49.53) (end 61.999999 50.130001) (width 1) (layer F.Cu) (net 18))
  (segment (start 61.999999 61.992237) (end 63.507762 63.5) (width 1) (layer F.Cu) (net 18))
  (segment (start 61.999999 50.130001) (end 61.999999 61.992237) (width 1) (layer F.Cu) (net 18))
  (segment (start 63.507762 63.5) (end 68.58 63.5) (width 1) (layer F.Cu) (net 18))
  (segment (start 68.58 63.5) (end 74.93 69.85) (width 1) (layer F.Cu) (net 18))
  (segment (start 74.93 73.91) (end 77.23 76.21) (width 1) (layer F.Cu) (net 18) (status 20))
  (segment (start 74.93 69.85) (end 74.93 73.91) (width 1) (layer F.Cu) (net 18))
  (segment (start 77.1 49.53) (end 74.63 49.53) (width 1) (layer F.Cu) (net 19) (status 20))
  (segment (start 77.47 65.405) (end 77.47 49.9) (width 1) (layer F.Cu) (net 19))
  (segment (start 79.756 67.691) (end 77.47 65.405) (width 1) (layer F.Cu) (net 19))
  (segment (start 82.33 76.21) (end 80.067999 73.947999) (width 1) (layer F.Cu) (net 19) (status 10))
  (segment (start 77.47 49.9) (end 77.1 49.53) (width 1) (layer F.Cu) (net 19))
  (segment (start 80.067999 73.947999) (end 80.043999 73.947999) (width 1) (layer F.Cu) (net 19))
  (segment (start 80.043999 73.947999) (end 79.756 73.66) (width 1) (layer F.Cu) (net 19))
  (segment (start 79.756 73.66) (end 79.756 67.691) (width 1) (layer F.Cu) (net 19))
  (segment (start 115.94 49.53) (end 118.41 49.53) (width 1) (layer F.Cu) (net 20) (status 20))
  (segment (start 115.060011 50.409989) (end 115.94 49.53) (width 1) (layer F.Cu) (net 20))
  (segment (start 115.060011 50.409989) (end 115.060011 65.632227) (width 1) (layer F.Cu) (net 20))
  (segment (start 115.060011 65.632227) (end 113.437773 65.632227) (width 1) (layer F.Cu) (net 20))
  (segment (start 113.437773 65.632227) (end 110.49 68.58) (width 1) (layer F.Cu) (net 20))
  (segment (start 110.49 73.55) (end 107.83 76.21) (width 1) (layer F.Cu) (net 20) (status 20))
  (segment (start 110.49 68.58) (end 110.49 73.55) (width 1) (layer F.Cu) (net 20))
  (segment (start 130.940001 50.030001) (end 130.44 49.53) (width 1) (layer F.Cu) (net 21))
  (segment (start 130.44 49.53) (end 127.97 49.53) (width 1) (layer F.Cu) (net 21) (status 20))
  (segment (start 130.940001 50.030001) (end 130.940001 60.829999) (width 1) (layer F.Cu) (net 21))
  (segment (start 124.962239 60.829999) (end 115.57 70.222238) (width 1) (layer F.Cu) (net 21))
  (segment (start 130.940001 60.829999) (end 124.962239 60.829999) (width 1) (layer F.Cu) (net 21))
  (segment (start 115.57 73.57) (end 112.93 76.21) (width 1) (layer F.Cu) (net 21) (status 20))
  (segment (start 115.57 70.222238) (end 115.57 73.57) (width 1) (layer F.Cu) (net 21))
  (segment (start 71.368001 75.448001) (end 72.13 76.21) (width 1) (layer F.Cu) (net 22) (status 20))
  (segment (start 71.003001 75.448001) (end 71.368001 75.448001) (width 1) (layer F.Cu) (net 22))
  (segment (start 69.85 74.295) (end 71.003001 75.448001) (width 1) (layer F.Cu) (net 22))
  (segment (start 62.679331 65.50001) (end 66.77001 65.50001) (width 1) (layer F.Cu) (net 22))
  (segment (start 54.31 49.53) (end 56.78 49.53) (width 1) (layer F.Cu) (net 22) (status 10))
  (segment (start 66.77001 65.50001) (end 69.85 68.58) (width 1) (layer F.Cu) (net 22))
  (segment (start 56.78 49.53) (end 59.69 52.44) (width 1) (layer F.Cu) (net 22))
  (segment (start 69.85 68.58) (end 69.85 74.295) (width 1) (layer F.Cu) (net 22))
  (segment (start 59.69 52.44) (end 59.69 62.510678) (width 1) (layer F.Cu) (net 22))
  (segment (start 59.69 62.510678) (end 62.679331 65.50001) (width 1) (layer F.Cu) (net 22))
  (segment (start 42.28 49.53) (end 44.75 49.53) (width 1) (layer F.Cu) (net 23) (status 20))
  (segment (start 41.91 49.9) (end 42.28 49.53) (width 1) (layer F.Cu) (net 23))
  (segment (start 44.45 64.77) (end 41.91 62.23) (width 1) (layer F.Cu) (net 23))
  (segment (start 58.937762 64.77) (end 44.45 64.77) (width 1) (layer F.Cu) (net 23))
  (segment (start 61.477762 67.31) (end 58.937762 64.77) (width 1) (layer F.Cu) (net 23))
  (segment (start 41.91 49.9) (end 41.91 62.23) (width 1) (layer F.Cu) (net 23))
  (segment (start 66.268001 75.448001) (end 66.268001 75.412001) (width 1) (layer F.Cu) (net 23))
  (segment (start 67.03 76.21) (end 66.268001 75.448001) (width 1) (layer F.Cu) (net 23) (status 10))
  (segment (start 66.268001 75.412001) (end 64.516 73.66) (width 1) (layer F.Cu) (net 23))
  (segment (start 64.516 73.66) (end 64.516 69.088) (width 1) (layer F.Cu) (net 23))
  (segment (start 62.738 67.31) (end 64.516 69.088) (width 1) (layer F.Cu) (net 23))
  (segment (start 61.477762 67.31) (end 62.738 67.31) (width 1) (layer F.Cu) (net 23))
  (segment (start 98.06 49.53) (end 100.53 49.53) (width 1) (layer F.Cu) (net 24) (status 20))
  (segment (start 97.63 49.96) (end 98.06 49.53) (width 1) (layer F.Cu) (net 24))
  (segment (start 97.63 76.21) (end 100.33 73.51) (width 1) (layer F.Cu) (net 24) (status 10))
  (segment (start 100.33 73.51) (end 100.33 64.135) (width 1) (layer F.Cu) (net 24))
  (segment (start 100.33 64.135) (end 97.63 61.435) (width 1) (layer F.Cu) (net 24))
  (segment (start 97.63 61.435) (end 97.63 49.96) (width 1) (layer F.Cu) (net 24))
  (segment (start 112.56 49.53) (end 110.09 49.53) (width 1) (layer F.Cu) (net 25) (status 20))
  (segment (start 113.060001 50.030001) (end 112.56 49.53) (width 1) (layer F.Cu) (net 25))
  (segment (start 113.060001 50.030001) (end 113.060001 61.564999) (width 1) (layer F.Cu) (net 25))
  (segment (start 113.060001 61.564999) (end 105.41 69.215) (width 1) (layer F.Cu) (net 25))
  (segment (start 105.41 73.53) (end 102.73 76.21) (width 1) (layer F.Cu) (net 25) (status 20))
  (segment (start 105.41 69.215) (end 105.41 73.53) (width 1) (layer F.Cu) (net 25))
  (segment (start 56.83 75.88) (end 56.83 76.21) (width 1) (layer F.Cu) (net 26))
  (segment (start 50.26001 69.31001) (end 56.83 75.88) (width 1) (layer F.Cu) (net 26))
  (segment (start 26.67 49.53) (end 22.86 49.53) (width 1) (layer F.Cu) (net 26))
  (segment (start 21.59 50.8) (end 21.59 59.69) (width 1) (layer F.Cu) (net 26))
  (segment (start 22.86 49.53) (end 21.59 50.8) (width 1) (layer F.Cu) (net 26))
  (segment (start 31.21001 69.31001) (end 50.26001 69.31001) (width 1) (layer F.Cu) (net 26))
  (segment (start 21.59 59.69) (end 31.21001 69.31001) (width 1) (layer F.Cu) (net 26))
  (segment (start 38.988441 49.53) (end 36.23 49.53) (width 1) (layer F.Cu) (net 27) (status 20))
  (segment (start 59.436 74.295) (end 59.436 68.616) (width 1) (layer F.Cu) (net 27))
  (segment (start 39.37 62.51844) (end 39.37 49.911559) (width 1) (layer F.Cu) (net 27))
  (segment (start 59.436 68.616) (end 58.13 67.31) (width 1) (layer F.Cu) (net 27))
  (segment (start 39.37 49.911559) (end 38.988441 49.53) (width 1) (layer F.Cu) (net 27))
  (segment (start 58.13 67.31) (end 44.16156 67.31) (width 1) (layer F.Cu) (net 27))
  (segment (start 44.16156 67.31) (end 39.37 62.51844) (width 1) (layer F.Cu) (net 27))
  (segment (start 60.589001 75.448001) (end 59.436 74.295) (width 1) (layer F.Cu) (net 27))
  (segment (start 61.168001 75.448001) (end 60.589001 75.448001) (width 1) (layer F.Cu) (net 27))
  (segment (start 61.93 76.21) (end 61.168001 75.448001) (width 1) (layer F.Cu) (net 27) (status 10))

  (zone (net 10) (net_name GNDA) (layer F.Cu) (tstamp 5CE3E6FF) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.7 12.7) (xy 182.88 12.7) (xy 182.88 78.74) (xy 12.7 78.74)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.13 41.275) (xy 166.37 41.275) (xy 168.91 43.18) (xy 168.91 66.04) (xy 166.37 68.58)
        (xy 142.875 68.58) (xy 134.62 77.47) (xy 55.88 77.47) (xy 52.07 74.295) (xy 34.925 74.295)
        (xy 24.13 63.5) (xy 24.13 43.18)
      )
    )
  )
  (zone (net 10) (net_name GNDA) (layer B.Cu) (tstamp 5CE3E6FC) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.5)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.7 12.7) (xy 182.88 12.7) (xy 182.88 78.74) (xy 12.7 78.74)
      )
    )
  )
)
