(footprint "Teensy41_pinheaders"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -10.16 0)
		(layer "F.SilkS")
		(uuid "2ddc51ed-ee0e-4dba-a3c8-c0f78f64c921")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Teensy 4.1"
		(at 0 10.16 0)
		(layer "F.Fab")
		(uuid "0c7f9889-acf0-4dda-b0ce-5665eb68d5d4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "066466b0-a6b6-46a7-bb8d-0d275aeadd8c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2a1b75cf-592e-4bfb-85c5-67e012cd6c38")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "91b836d3-2dfa-41c8-b231-959b96d376e1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -31.75 -3.81)
		(end -30.48 -3.81)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9b404f59-8828-4260-8a17-8d59c3aa70eb")
	)
	(fp_line
		(start -31.75 3.81)
		(end -31.75 -3.81)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7ee1a88c-c81b-42f2-94e6-f9a972639ad6")
	)
	(fp_line
		(start -30.48 -8.89)
		(end 30.48 -8.89)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4fd39068-31d4-4944-b765-89ddd60a7763")
	)
	(fp_line
		(start -30.48 3.81)
		(end -31.75 3.81)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c1fff68d-168e-473c-85ee-59b4e83850f5")
	)
	(fp_line
		(start -30.48 8.89)
		(end -30.48 -8.89)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "34c5204f-ee58-4076-a4d9-b854a0232e00")
	)
	(fp_line
		(start 29.21 -5.08)
		(end 29.21 5.08)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "dc7cae27-5068-4b0a-90a5-0d5419117201")
	)
	(fp_line
		(start 29.21 5.08)
		(end 30.48 5.08)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "47a1b8ee-34d2-4bb2-be12-5252e1ccefd6")
	)
	(fp_line
		(start 30.48 -8.89)
		(end 30.48 8.89)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "398a80cf-c9ec-482d-980d-fca02ef4bff5")
	)
	(fp_line
		(start 30.48 -5.08)
		(end 29.21 -5.08)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "cf78f3ec-a7d8-4a9f-ae32-05efbdf0a699")
	)
	(fp_line
		(start 30.48 8.89)
		(end -30.48 8.89)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6f9abf68-9fb2-4d23-8044-0ed97e57c1c8")
	)
	(fp_text user "USB"
		(at -29.5 0 -90)
		(layer "F.SilkS")
		(uuid "2a0240e4-f4fd-4185-9540-0e3f1c1f2e24")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "Micro SD"
		(at 24.13 0 0)
		(layer "F.SilkS")
		(uuid "d6570f18-55f2-477b-9e96-633f7325682e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at -29.21 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "408e10b9-f94e-4cc1-9c3c-5de5c7f2e1bc")
	)
	(pad "2" thru_hole circle
		(at -26.67 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7add8b5f-a982-417e-a032-51c54dfceb6b")
	)
	(pad "3" thru_hole circle
		(at -24.13 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4bc46af8-dd63-4657-a55d-6f0a1102dd55")
	)
	(pad "4" thru_hole circle
		(at -21.59 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "60f0e200-4110-4199-8f6e-b87b548ef2ba")
	)
	(pad "5" thru_hole circle
		(at -19.05 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "770718ea-4bc8-44a2-b88f-81d2d8989789")
	)
	(pad "6" thru_hole circle
		(at -16.51 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2ef68cf4-fc42-46d8-a369-bd7c99d61bfe")
	)
	(pad "7" thru_hole circle
		(at -13.97 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a72f9bc9-c3f6-4b63-8af4-8cdc62461ecb")
	)
	(pad "8" thru_hole circle
		(at -11.43 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a7e65299-9e86-44d3-9a57-bc9e74c2f1a3")
	)
	(pad "9" thru_hole circle
		(at -8.89 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "48a8c25c-254c-4bcb-9446-00a18330933e")
	)
	(pad "10" thru_hole circle
		(at -6.35 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5e80db9b-2656-4a02-94e8-b0e1b64814ca")
	)
	(pad "11" thru_hole circle
		(at -3.81 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "52d760a3-8eac-481c-9007-e2a461a70359")
	)
	(pad "12" thru_hole circle
		(at -1.27 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "57487f3f-c134-4d01-86b5-7d095b481745")
	)
	(pad "13" thru_hole circle
		(at 1.27 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ac1c4b83-2f7e-439a-b627-bdd9b5f22c9e")
	)
	(pad "14" thru_hole circle
		(at 3.81 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ca2343ce-1bce-499c-80d9-2f5ddab78bea")
	)
	(pad "15" thru_hole circle
		(at 6.35 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0957c39d-1654-4c30-a02b-0a60287b2ae3")
	)
	(pad "16" thru_hole circle
		(at 8.89 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fd8cdce1-dac6-4658-a56a-a1905167bdaa")
	)
	(pad "17" thru_hole circle
		(at 11.43 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3064c417-5da9-4335-94b5-35ac46ac40f1")
	)
	(pad "18" thru_hole circle
		(at 13.97 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "82539798-b4d0-43b4-bdd4-ea8185fd7abe")
	)
	(pad "19" thru_hole circle
		(at 16.51 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3d39c814-46e1-4ebe-a97b-b71baf7a7779")
	)
	(pad "20" thru_hole circle
		(at 19.05 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f929844c-e777-4233-9dec-1e3b5c6b5ba1")
	)
	(pad "21" thru_hole circle
		(at 21.59 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "48e8a972-edb7-4d1d-9ea4-2922c1480ed7")
	)
	(pad "22" thru_hole circle
		(at 24.13 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5d47d7ca-17f5-4c62-84c4-0bba1f2bc56b")
	)
	(pad "23" thru_hole circle
		(at 26.67 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4de98cd3-8e42-4b9d-9342-b3c14a9fbcce")
	)
	(pad "24" thru_hole circle
		(at 29.21 7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "df449a78-becd-425a-90fb-d44e63e90b95")
	)
	(pad "25" thru_hole circle
		(at 29.21 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f633b66b-1f13-4a05-9afb-47a105632997")
	)
	(pad "26" thru_hole circle
		(at 26.67 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "09a06a0c-3dc1-490b-9c2c-4d699009d1e2")
	)
	(pad "27" thru_hole circle
		(at 24.13 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d54e2b96-34d2-466d-8d1d-3abfe7374505")
	)
	(pad "28" thru_hole circle
		(at 21.59 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9fb9c534-a60d-41dd-8136-3a520b5dce44")
	)
	(pad "29" thru_hole circle
		(at 19.05 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4f48a7b8-6e19-4d9b-8e1c-23f255808880")
	)
	(pad "30" thru_hole circle
		(at 16.51 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2094a7ee-6da7-4db1-a3a1-37bf3301076d")
	)
	(pad "31" thru_hole circle
		(at 13.97 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "84130ee3-8050-45b0-aa70-72b2eb71f363")
	)
	(pad "32" thru_hole circle
		(at 11.43 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "533e5af0-30ff-4d50-8fd6-99ff6c03d8cd")
	)
	(pad "33" thru_hole circle
		(at 8.89 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d3a337d4-cbd6-4169-821b-71b7ddf273ae")
	)
	(pad "34" thru_hole circle
		(at 6.35 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9160cdb7-1e32-411f-874c-b63b8c422329")
	)
	(pad "35" thru_hole circle
		(at 3.81 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "831318d2-a37d-4749-bb0e-2fccaf9222cb")
	)
	(pad "36" thru_hole circle
		(at 1.27 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2075ebc8-afdf-4414-a93d-c94d3b492e0d")
	)
	(pad "37" thru_hole circle
		(at -1.27 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9ec7a1bb-9409-4d9b-9241-a6ea47d0139b")
	)
	(pad "38" thru_hole circle
		(at -3.81 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "50494e76-1f1e-467e-8689-841d62182686")
	)
	(pad "39" thru_hole circle
		(at -6.35 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b6087078-c902-4821-8f7d-74beae97c78a")
	)
	(pad "40" thru_hole circle
		(at -8.89 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "04be0499-6a5b-456b-9096-76cfdc2d3d3f")
	)
	(pad "41" thru_hole circle
		(at -11.43 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "338b62f2-e54e-4892-9fda-53d398a1b9dd")
	)
	(pad "42" thru_hole circle
		(at -13.97 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "58144715-be8b-4f63-8bf5-318f2809dd84")
	)
	(pad "43" thru_hole circle
		(at -16.51 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "736eca43-ec1d-445c-a9be-a42422533757")
	)
	(pad "44" thru_hole circle
		(at -19.05 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d6284b12-01af-4fbe-903c-e5369af44ea1")
	)
	(pad "45" thru_hole circle
		(at -21.59 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "96526a4e-7e51-40dd-a496-d99d29fa703a")
	)
	(pad "46" thru_hole circle
		(at -24.13 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0e93da91-a4f3-4012-8902-e0f243d7ccde")
	)
	(pad "47" thru_hole circle
		(at -26.67 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ced17b42-9b30-4846-95af-d46394e75c0c")
	)
	(pad "48" thru_hole circle
		(at -29.21 -7.62)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c615adab-fa03-45ee-a665-2e76df1c011e")
	)
	(pad "50" thru_hole circle
		(at 16.51 5.08)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "287e21d1-102a-4bac-a6d8-932dd741de4a")
	)
	(pad "51" thru_hole circle
		(at 16.51 2.54)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f249ca39-deaf-4d9d-a1c9-528271938bf3")
	)
	(pad "52" thru_hole circle
		(at 16.51 0)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a4738b91-70f7-4bcb-93d3-fcd50d22fbe3")
	)
	(pad "53" thru_hole circle
		(at 16.51 -2.54)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5c15b375-c6c1-4060-a7e4-5b48ca5dcac6")
	)
	(pad "54" thru_hole circle
		(at 16.51 -5.08)
		(size 1.6 1.6)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "306c8b7d-6f3b-4ddd-a1b0-5460863cf2ff")
	)
	(model "${KICAD_USER_DIR}/teensy.pretty/Teensy_4.1_Assembly.STEP"
		(offset
			(xyz 0 0 0.762)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
